630 1760609827324 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is NOT null
630 1760609827324 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9012, AttachedToolVID = 4d8
630 1760609827324 GEN4_CONNECT_DIAGNOSTICS:transport type = USB
630 1760609827324 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9012, AttachedToolVID = 4d8
630 1760609827365 com.microchip.mplab.mdbcore.RealICETool.RIDbgToolCom
630 1760609827365 GEN4_CONNECT_DIAGNOSTICS:Before MPLABCommTool.Connect()
630 1760609827365 GEN4_CONNECT_DIAGNOSTICS:After MPLABCommTool.Connect()
630 1760609827365 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool.Connect() returned MPLABCOMM_NO_ERROR
630 1760609827366 GEN4_CONNECT_DIAGNOSTICS:Attaching to MPLABCommTool plugnplay
630 1760609827375 GEN4_CONNECT_DIAGNOSTICS:Adding new plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@374b45a9
630 1760609827375 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
630 1760609827375 GEN4_CONNECT_DIAGNOSTICS:com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@374b45a9
630 1760609827375 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
630 1760609827377 GEN4_CONNECT_DIAGNOSTICS:Registering for alternate PNP notifications. CommPnPCriteria.cPIDList = [2177, 2179, 217a, 2141, 9017, 901b, 9036, 9035], CommPnPCriteria.cSerialNumber = bur213375184

630 1760609827686 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:init
630 1760609827686 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
630 1760609827686 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: Values:
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: pcAddress = 7fffffffffffffff, Vpp = 3.30, useRowEraseIfVoltageIsLow = false, voltageBelowWhichUseRowErase = 0.00, deviceName = PIC32MX270F256B, programmerType = PIC32MX_JTAG_ONLY
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: MemInfo values:
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = ffffffff, exists = true, startAddr = 1d000000, endAddr = 1d03ffff, rowSize = 0400, rowEraseSize = 0400, addrInc = 0004, widthProgram = 0004
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = ffffffff, exists = true, startAddr = 1fc00bf0, endAddr = 1fc00bff, rowSize = 0001, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = true, startAddr = 00000000, endAddr = 00000000, rowSize = 0400, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0400, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = ffffffff, exists = true, startAddr = 1f800000, endAddr = 1f886fff, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 7fffffff, exists = true, startAddr = ffffffff, endAddr = fffffffe, rowSize = 0001, rowEraseSize = 0000, addrInc = 0001, widthProgram = 0001
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
630 1760609827687 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: CfgRequiredBitsMask Values:
630 1760609827688 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Address = 1fc00bf0, Mask = f000ffff
630 1760609827688 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Address = 1fc00bf4, Mask = 00078777
630 1760609827688 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Address = 1fc00bf8, Mask = 03dff7a7
630 1760609827688 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Address = 1fc00bfc, Mask = 1107fc1c
630 1760609827688 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B BasicInfo: Values:
630 1760609827688 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B BasicInfo: InputStream = com.microchip.mplab.libs.toolpacksupport.EquatableFileInputStream@1fa17626, ToolFlavor = PICKit4
630 1760609827688 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830029 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:init
630 1760609830029 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830029 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B none
630 1760609830029 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

630 1760609830029 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
630 1760609830029 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
630 1760609830029 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B RI4DebugInterface
630 1760609830029 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830029 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
630 1760609830029 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830029 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.RI4ToolsController.implementations.RI4DebugInterfaceImpl@313a7a59
630 1760609830029 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

630 1760609830044 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
630 1760609830044 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
630 1760609830044 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B RI4ProgramInterface
630 1760609830044 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830044 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
630 1760609830044 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830044 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ProgramInterfaceImpl@40c7898c
630 1760609830044 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

630 1760609830057 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
630 1760609830057 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
630 1760609830057 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B RI4ConnectInterface
630 1760609830057 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830058 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
630 1760609830058 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830058 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.PK4ToolsController.PK4ConnectInterfaceImpl@232282da
630 1760609830058 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End
630 1760609830063 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]
630 1760609830063 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
630 1760609830063 GEN4_CONNECT_DIAGNOSTICS:Setting selected tool type to pk4
630 1760609830063 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
630 1760609830063 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]

630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:selectCore
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B PIC32MX270F256B
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:selectCore
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B none
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B RI4ControllerDiagnosticsInterface
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ControllerDiagnosticsInterfaceImpl@654ef5d8
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B ProgrammerToGo
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.RI4ToolsController.implementations.ProgrammerToGoImpl@ac414fd
630 1760609830065 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

630 1760609830066 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
630 1760609830066 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
630 1760609830066 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Status
630 1760609830066 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830066 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
630 1760609830066 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830066 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B null
630 1760609830066 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

630 1760609830074 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Pre:SetProgramExec
630 1760609830074 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload
630 1760609830075 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B FileRegs
630 1760609830075 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B a0000900
630 1760609830075 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Length = 1688
630 1760609830075 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload End
630 1760609830075 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Post:SetProgramExec
630 1760609830075 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return Value
630 1760609830075 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B true
630 1760609830075 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return End
630 1760609830075 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
630 1760609830075 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@142bffef
630 1760609830076 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
630 1760609830078 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
630 1760609830078 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
630 1760609830078 GEN4_CONNECT_DIAGNOSTICS:uMode = checkingVersions
630 1760609830078 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
630 1760609830078 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
630 1760609830078 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
630 1760609830078 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:Parsing file  for firmware updates
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ParseSelectedVersionsFromJamFile()
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:Jame file line = boot.hex,010000
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:Jame file line = scripts.xml,000671
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app1 020135, 0040C000
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app2 1.15.20, 00500000
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app3 000000, FFFFFFFF
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app4 000000, FFFFFFFF
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app5 000000, FFFFFFFF
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app6 000000, FFFFFFFF
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app7 000000, FFFFFFFF
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app8 000000, FFFFFFFF
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ri4ParseSelectedVersionsFromJamFile()
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
630 1760609830079 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4

630 1760609830079 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:EstablishCommunincations
630 1760609830079 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
630 1760609830079 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B com.microchip.mplab.mdbcore.PK4Tool.PK4Com@1c389717
630 1760609830079 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830084 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:EstablishCommunincations
630 1760609830084 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830084 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B true
630 1760609830084 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

630 1760609830085 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:GetFirmwareInfo
630 1760609830085 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
630 1760609830085 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B null
630 1760609830085 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830093 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:GetFirmwareInfo
630 1760609830093 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830093 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: Values:
630 1760609830093 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
630 1760609830093 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End
630 1760609830099 GEN4_CONNECT_DIAGNOSTICS:appNeedsUpdate returned false
630 1760609830099 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

630 1760609830099 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:EstablishCommunincations
630 1760609830099 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
630 1760609830099 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B com.microchip.mplab.mdbcore.PK4Tool.PK4Com@1c389717
630 1760609830099 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830100 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:EstablishCommunincations
630 1760609830100 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830100 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B true
630 1760609830100 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

630 1760609830100 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:GetFirmwareInfo
630 1760609830100 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
630 1760609830100 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B null
630 1760609830100 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830107 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:GetFirmwareInfo
630 1760609830107 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830107 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: Values:
630 1760609830107 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
630 1760609830107 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

630 1760609830107 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:GetFirmwareInfo
630 1760609830107 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
630 1760609830107 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B null
630 1760609830107 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830115 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:GetFirmwareInfo
630 1760609830115 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830115 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: Values:
630 1760609830115 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
630 1760609830115 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End
630 1760609830117 XXXX 1760609830117, Thread 630: XXXX 1760609830117, Entering Thread 630: Commands::runScriptWithUpload with script contents. contents[0] = 0x5e, ...  
630 1760609830118 XXXX 1760609830118, Thread 630: XXXX 1760609830118, Entering Thread 630: ToolCommUsb::readTransfer, sideData is 0xd bytes long, transferDataLength is 0x4 bytes long  
630 1760609830121 XXXX 1760609830121, Thread 630: XXXX 1760609830121, Exiting Thread 630: ToolCommUsb::readTransfer,  cr.status = 0x0  
630 1760609830121 XXXX 1760609830121, Thread 630: XXXX 1760609830121, Exiting Thread 630: Commands::runScriptWithUpload  
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@142bffef
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:uMode = done
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:Don't upgrade fimware = false
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
630 1760609830122 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

630 1760609830123 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:SetPowerInfo
630 1760609830123 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
630 1760609830123 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B PowerInfo: Values:
630 1760609830123 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B PowerInfo: shotDownSystem = false, isToolPower = true, voltage = 3.250000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
630 1760609830123 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830123 XXXX 1760609830123, Thread 630: XXXX 1760609830123, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
630 1760609830123 XXXX 1760609830123, Thread 630: XXXX 1760609830123, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830123 XXXX 1760609830123, Thread 630: XXXX 1760609830123, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
630 1760609830124 XXXX 1760609830124, Thread 630: XXXX 1760609830124, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830124 XXXX 1760609830124, Thread 630: XXXX 1760609830124, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
630 1760609830136 XXXX 1760609830136, Thread 630: XXXX 1760609830136, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830136 XXXX 1760609830136, Thread 630: XXXX 1760609830136, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
630 1760609830313 XXXX 1760609830313, Thread 630: XXXX 1760609830313, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830313 XXXX 1760609830313, Thread 630: XXXX 1760609830313, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
630 1760609830318 XXXX 1760609830318, Thread 630: XXXX 1760609830318, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830318 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:SetPowerInfo
630 1760609830318 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830318 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B none
630 1760609830318 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

630 1760609830318 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:SetLEDBrightness
630 1760609830318 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
630 1760609830318 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B 5
630 1760609830318 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830318 XXXX 1760609830318, Thread 630: XXXX 1760609830318, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0xcf, ...  
630 1760609830319 XXXX 1760609830319, Thread 630: XXXX 1760609830319, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830319 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:SetLEDBrightness
630 1760609830319 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830319 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B none
630 1760609830319 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

630 1760609830319 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:SetToolInfo
630 1760609830319 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
630 1760609830319 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B ToolInfo: Values:
630 1760609830320 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B ToolInfo: speedLevel = 1, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
630 1760609830320 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830320 XXXX 1760609830320, Thread 630: XXXX 1760609830320, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
630 1760609830321 XXXX 1760609830321, Thread 630: XXXX 1760609830321, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830321 XXXX 1760609830321, Thread 630: XXXX 1760609830321, Entering Thread 630: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
630 1760609830322 XXXX 1760609830322, Thread 630: XXXX 1760609830322, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830322 XXXX 1760609830322, Thread 630: XXXX 1760609830322, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
630 1760609830323 XXXX 1760609830323, Thread 630: XXXX 1760609830323, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830323 XXXX 1760609830323, Thread 630: XXXX 1760609830323, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0xec, ...  
630 1760609830324 XXXX 1760609830324, Thread 630: XXXX 1760609830324, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830324 XXXX 1760609830324, Thread 630: XXXX 1760609830324, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
630 1760609830325 XXXX 1760609830325, Thread 630: XXXX 1760609830325, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830325 XXXX 1760609830325, Thread 630: XXXX 1760609830325, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
630 1760609830326 XXXX 1760609830326, Thread 630: XXXX 1760609830326, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830326 XXXX 1760609830326, Thread 630: XXXX 1760609830326, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
630 1760609830327 XXXX 1760609830327, Thread 630: XXXX 1760609830327, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830327 XXXX 1760609830327, Thread 630: XXXX 1760609830327, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
630 1760609830329 XXXX 1760609830329, Thread 630: XXXX 1760609830329, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830329 XXXX 1760609830329, Thread 630: XXXX 1760609830329, Entering Thread 630: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
630 1760609830330 XXXX 1760609830330, Thread 630: XXXX 1760609830330, Exiting Thread 630: Commands::runScriptBasic  
630 1760609830330 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:SetToolInfo
630 1760609830330 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
630 1760609830330 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B none
630 1760609830330 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

630 1760609830331 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:GetTargetIDInfo
630 1760609830331 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
630 1760609830331 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B null
630 1760609830331 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
630 1760609830332 XXXX 1760609830332, Thread 630: com.Send returned false 
