598 1759239991791 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is NOT null
598 1759239991791 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9012, AttachedToolVID = 4d8
598 1759239991791 GEN4_CONNECT_DIAGNOSTICS:transport type = USB
598 1759239991791 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9012, AttachedToolVID = 4d8
598 1759239991850 com.microchip.mplab.mdbcore.RealICETool.RIDbgToolCom
598 1759239991850 GEN4_CONNECT_DIAGNOSTICS:Before MPLABCommTool.Connect()
598 1759239991850 GEN4_CONNECT_DIAGNOSTICS:After MPLABCommTool.Connect()
598 1759239991850 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool.Connect() returned MPLABCOMM_NO_ERROR
598 1759239991851 GEN4_CONNECT_DIAGNOSTICS:Attaching to MPLABCommTool plugnplay
598 1759239991863 GEN4_CONNECT_DIAGNOSTICS:Adding new plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@4dcd7401
598 1759239991863 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
598 1759239991863 GEN4_CONNECT_DIAGNOSTICS:com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@4dcd7401
598 1759239991863 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
598 1759239991865 GEN4_CONNECT_DIAGNOSTICS:Registering for alternate PNP notifications. CommPnPCriteria.cPIDList = [2177, 2179, 217a, 2141, 9017, 901b, 9036, 9035], CommPnPCriteria.cSerialNumber = bur213375184

598 1759239992306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:init
598 1759239992306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: Values:
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: pcAddress = 7fffffffffffffff, Vpp = 3.30, useRowEraseIfVoltageIsLow = false, voltageBelowWhichUseRowErase = 0.00, deviceName = PIC32MX270F256B, programmerType = PIC32MX_JTAG_ONLY
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: MemInfo values:
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = ffffffff, exists = true, startAddr = 1d000000, endAddr = 1d03ffff, rowSize = 0400, rowEraseSize = 0400, addrInc = 0004, widthProgram = 0004
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = ffffffff, exists = true, startAddr = 1fc00bf0, endAddr = 1fc00bff, rowSize = 0001, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = true, startAddr = 00000000, endAddr = 00000000, rowSize = 0400, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0400, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = ffffffff, exists = true, startAddr = 1f800000, endAddr = 1f886fff, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 7fffffff, exists = true, startAddr = ffffffff, endAddr = fffffffe, rowSize = 0001, rowEraseSize = 0000, addrInc = 0001, widthProgram = 0001
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
598 1759239992307 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: CfgRequiredBitsMask Values:
598 1759239992308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Address = 1fc00bf0, Mask = f000ffff
598 1759239992308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Address = 1fc00bf4, Mask = 00078777
598 1759239992308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Address = 1fc00bf8, Mask = 03dff7a7
598 1759239992308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Address = 1fc00bfc, Mask = 1107fc1c
598 1759239992308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B BasicInfo: Values:
598 1759239992308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B BasicInfo: InputStream = com.microchip.mplab.libs.toolpacksupport.EquatableFileInputStream@1fa17626, ToolFlavor = PICKit4
598 1759239992308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:init
598 1759239995323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B none
598 1759239995323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

598 1759239995323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
598 1759239995323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
598 1759239995323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B RI4DebugInterface
598 1759239995323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
598 1759239995323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.RI4ToolsController.implementations.RI4DebugInterfaceImpl@62857e32
598 1759239995323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

598 1759239995339 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
598 1759239995339 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
598 1759239995339 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B RI4ProgramInterface
598 1759239995339 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995339 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
598 1759239995339 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995339 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ProgramInterfaceImpl@48fe462
598 1759239995339 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

598 1759239995352 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
598 1759239995352 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
598 1759239995352 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B RI4ConnectInterface
598 1759239995352 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995353 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
598 1759239995353 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995353 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.PK4ToolsController.PK4ConnectInterfaceImpl@3e39ee6c
598 1759239995353 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End
598 1759239995359 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]
598 1759239995359 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
598 1759239995359 GEN4_CONNECT_DIAGNOSTICS:Setting selected tool type to pk4
598 1759239995359 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
598 1759239995359 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]

598 1759239995360 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:selectCore
598 1759239995360 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
598 1759239995360 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B PIC32MX270F256B
598 1759239995360 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:selectCore
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B none
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B RI4ControllerDiagnosticsInterface
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ControllerDiagnosticsInterfaceImpl@5d29f8ea
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B ProgrammerToGo
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.RI4ToolsController.implementations.ProgrammerToGoImpl@5c91b839
598 1759239995361 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

598 1759239995362 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
598 1759239995362 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
598 1759239995362 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Status
598 1759239995362 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995362 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
598 1759239995362 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995362 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B null
598 1759239995362 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

598 1759239995368 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Pre:SetProgramExec
598 1759239995368 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload
598 1759239995369 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B FileRegs
598 1759239995369 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B a0000900
598 1759239995369 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Length = 1688
598 1759239995369 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload End
598 1759239995369 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Post:SetProgramExec
598 1759239995369 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return Value
598 1759239995369 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B true
598 1759239995369 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return End
598 1759239995369 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
598 1759239995369 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@522f0a93
598 1759239995369 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
598 1759239995371 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
598 1759239995371 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
598 1759239995371 GEN4_CONNECT_DIAGNOSTICS:uMode = checkingVersions
598 1759239995371 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
598 1759239995371 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
598 1759239995371 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
598 1759239995371 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:Parsing file  for firmware updates
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ParseSelectedVersionsFromJamFile()
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:Jame file line = boot.hex,010000
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:Jame file line = scripts.xml,000671
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app1 020135, 0040C000
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app2 1.15.20, 00500000
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app3 000000, FFFFFFFF
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app4 000000, FFFFFFFF
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app5 000000, FFFFFFFF
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app6 000000, FFFFFFFF
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app7 000000, FFFFFFFF
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app8 000000, FFFFFFFF
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ri4ParseSelectedVersionsFromJamFile()
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
598 1759239995372 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4

598 1759239995372 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:EstablishCommunincations
598 1759239995372 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
598 1759239995372 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B com.microchip.mplab.mdbcore.PK4Tool.PK4Com@14c38024
598 1759239995372 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:EstablishCommunincations
598 1759239995377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B true
598 1759239995377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

598 1759239995377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:GetFirmwareInfo
598 1759239995377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
598 1759239995377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B null
598 1759239995377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995386 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:GetFirmwareInfo
598 1759239995386 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995386 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: Values:
598 1759239995387 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
598 1759239995387 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End
598 1759239995393 GEN4_CONNECT_DIAGNOSTICS:appNeedsUpdate returned false
598 1759239995393 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

598 1759239995393 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:EstablishCommunincations
598 1759239995393 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
598 1759239995393 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B com.microchip.mplab.mdbcore.PK4Tool.PK4Com@14c38024
598 1759239995393 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995393 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:EstablishCommunincations
598 1759239995393 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995393 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B true
598 1759239995393 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

598 1759239995394 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:GetFirmwareInfo
598 1759239995394 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
598 1759239995394 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B null
598 1759239995394 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995401 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:GetFirmwareInfo
598 1759239995401 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995401 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: Values:
598 1759239995401 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
598 1759239995401 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

598 1759239995402 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:GetFirmwareInfo
598 1759239995402 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
598 1759239995402 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B null
598 1759239995402 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995409 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:GetFirmwareInfo
598 1759239995409 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995409 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: Values:
598 1759239995409 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
598 1759239995409 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End
598 1759239995411 XXXX 1759239995411, Thread 598: XXXX 1759239995411, Entering Thread 598: Commands::runScriptWithUpload with script contents. contents[0] = 0x5e, ...  
598 1759239995412 XXXX 1759239995412, Thread 598: XXXX 1759239995412, Entering Thread 598: ToolCommUsb::readTransfer, sideData is 0xd bytes long, transferDataLength is 0x4 bytes long  
598 1759239995416 XXXX 1759239995416, Thread 598: XXXX 1759239995416, Exiting Thread 598: ToolCommUsb::readTransfer,  cr.status = 0x0  
598 1759239995416 XXXX 1759239995416, Thread 598: XXXX 1759239995416, Exiting Thread 598: Commands::runScriptWithUpload  
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@522f0a93
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:uMode = done
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:Don't upgrade fimware = false
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
598 1759239995416 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

598 1759239995417 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:SetPowerInfo
598 1759239995417 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
598 1759239995417 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B PowerInfo: Values:
598 1759239995417 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B PowerInfo: shotDownSystem = false, isToolPower = true, voltage = 3.250000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
598 1759239995417 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995417 XXXX 1759239995417, Thread 598: XXXX 1759239995417, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
598 1759239995418 XXXX 1759239995418, Thread 598: XXXX 1759239995418, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995418 XXXX 1759239995418, Thread 598: XXXX 1759239995418, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
598 1759239995419 XXXX 1759239995419, Thread 598: XXXX 1759239995419, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995419 XXXX 1759239995419, Thread 598: XXXX 1759239995419, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
598 1759239995431 XXXX 1759239995431, Thread 598: XXXX 1759239995431, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995431 XXXX 1759239995431, Thread 598: XXXX 1759239995431, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
598 1759239995607 XXXX 1759239995607, Thread 598: XXXX 1759239995607, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995607 XXXX 1759239995607, Thread 598: XXXX 1759239995607, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
598 1759239995613 XXXX 1759239995613, Thread 598: XXXX 1759239995613, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995613 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:SetPowerInfo
598 1759239995613 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995613 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B none
598 1759239995613 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

598 1759239995613 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:SetLEDBrightness
598 1759239995613 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
598 1759239995613 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B 5
598 1759239995613 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995613 XXXX 1759239995613, Thread 598: XXXX 1759239995613, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0xcf, ...  
598 1759239995614 XXXX 1759239995614, Thread 598: XXXX 1759239995614, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995614 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:SetLEDBrightness
598 1759239995614 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995614 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B none
598 1759239995614 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

598 1759239995614 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:SetToolInfo
598 1759239995614 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
598 1759239995614 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B ToolInfo: Values:
598 1759239995614 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B ToolInfo: speedLevel = 1, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
598 1759239995614 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995614 XXXX 1759239995614, Thread 598: XXXX 1759239995614, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
598 1759239995615 XXXX 1759239995615, Thread 598: XXXX 1759239995615, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995615 XXXX 1759239995615, Thread 598: XXXX 1759239995615, Entering Thread 598: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
598 1759239995616 XXXX 1759239995616, Thread 598: XXXX 1759239995616, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995616 XXXX 1759239995616, Thread 598: XXXX 1759239995616, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
598 1759239995617 XXXX 1759239995617, Thread 598: XXXX 1759239995617, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995617 XXXX 1759239995617, Thread 598: XXXX 1759239995617, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0xec, ...  
598 1759239995618 XXXX 1759239995618, Thread 598: XXXX 1759239995618, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995618 XXXX 1759239995618, Thread 598: XXXX 1759239995618, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
598 1759239995619 XXXX 1759239995619, Thread 598: XXXX 1759239995619, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995619 XXXX 1759239995619, Thread 598: XXXX 1759239995619, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
598 1759239995621 XXXX 1759239995621, Thread 598: XXXX 1759239995621, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995621 XXXX 1759239995621, Thread 598: XXXX 1759239995621, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
598 1759239995622 XXXX 1759239995622, Thread 598: XXXX 1759239995622, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995622 XXXX 1759239995622, Thread 598: XXXX 1759239995622, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
598 1759239995623 XXXX 1759239995623, Thread 598: XXXX 1759239995623, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995623 XXXX 1759239995623, Thread 598: XXXX 1759239995623, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
598 1759239995624 XXXX 1759239995624, Thread 598: XXXX 1759239995624, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995624 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:SetToolInfo
598 1759239995624 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995624 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B none
598 1759239995624 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

598 1759239995626 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:GetTargetIDInfo
598 1759239995626 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
598 1759239995626 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B null
598 1759239995626 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
598 1759239995628 XXXX 1759239995628, Thread 598: XXXX 1759239995628, Entering Thread 598: Commands::runScriptBasic, script name = ReadDeviceParameters, timeOut = -1 ms  
598 1759239995629 XXXX 1759239995629, Thread 598: XXXX 1759239995629, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995629 XXXX 1759239995629, Thread 598: XXXX 1759239995629, Entering Thread 598: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
598 1759239995634 XXXX 1759239995634, Thread 598: XXXX 1759239995634, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995634 XXXX 1759239995634, Thread 598: XXXX 1759239995634, Entering Thread 598: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
598 1759239995635 XXXX 1759239995635, Thread 598: XXXX 1759239995635, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995635 XXXX 1759239995635, Thread 598: XXXX 1759239995635, Entering Thread 598: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
598 1759239995636 XXXX 1759239995636, Thread 598: XXXX 1759239995636, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995636 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:GetTargetIDInfo
598 1759239995636 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
598 1759239995636 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B TargetIDInfo: Values:
598 1759239995636 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B TargetIDInfo: DeviceID = 26600053
598 1759239995636 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

598 1759239995664 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Pre:SendOperation
598 1759239995664 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload
598 1759239995664 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B OperationInfo: Values:
598 1759239995665 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B OperationInfo: Type = erase, Mask = 00000000, Erase = false, Production Mode = true
598 1759239995665 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B TransferInfo: Start = 1d000000, End = 1d03ffff, Buffer Length = 0, Type = Pgm, Mask = 00000000
598 1759239995665 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B TransferInfo: Start = 1fc00bf0, End = 1fc00bff, Buffer Length = 0, Type = Cfg, Mask = 00000000
598 1759239995665 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B TransferInfo: Start = 1fc00000, End = 1fc00bef, Buffer Length = 0, Type = BootFlash, Mask = 00000000
598 1759239995665 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload End
598 1759239995665 XXXX 1759239995665, Thread 598: XXXX 1759239995665, Entering Thread 598: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
598 1759239995671 XXXX 1759239995671, Thread 598: XXXX 1759239995671, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995671 XXXX 1759239995671, Thread 598: XXXX 1759239995671, Entering Thread 598: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
598 1759239995672 XXXX 1759239995672, Thread 598: XXXX 1759239995672, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995672 XXXX 1759239995672, Thread 598: XXXX 1759239995672, Entering Thread 598: Commands::runScriptBasic, script name = EraseChip, timeOut = 30000 ms  
598 1759239995773 XXXX 1759239995773, Thread 598: XXXX 1759239995773, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995773 XXXX 1759239995773, Thread 598: XXXX 1759239995773, Entering Thread 598: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
598 1759239995774 XXXX 1759239995774, Thread 598: XXXX 1759239995774, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995774 XXXX 1759239995774, Thread 598: XXXX 1759239995774, Entering Thread 598: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
598 1759239995781 XXXX 1759239995781, Thread 598: XXXX 1759239995781, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995781 XXXX 1759239995781, Thread 598: XXXX 1759239995781, Entering Thread 598: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
598 1759239995781 XXXX 1759239995781, Thread 598: XXXX 1759239995781, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995781 XXXX 1759239995781, Thread 598: XXXX 1759239995781, Entering Thread 598: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
598 1759239995782 XXXX 1759239995782, Thread 598: XXXX 1759239995782, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995782 XXXX 1759239995782, Thread 598: XXXX 1759239995782, Entering Thread 598: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
598 1759239995783 XXXX 1759239995783, Thread 598: XXXX 1759239995783, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995783 XXXX 1759239995783, Thread 598: XXXX 1759239995783, Entering Thread 598: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
598 1759239995784 XXXX 1759239995784, Thread 598: XXXX 1759239995784, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995784 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Post:SendOperation
598 1759239995784 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return Value
598 1759239995784 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B None
598 1759239995784 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return End

598 1759239995789 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Pre:SendOperation
598 1759239995789 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload
598 1759239995789 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B OperationInfo: Values:
598 1759239995789 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B OperationInfo: Type = write, Mask = 00000000, Erase = false, Production Mode = true
598 1759239995789 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B TransferInfo: Start = 1d000000, End = 1d013fff, Buffer Length = 81920, Type = Pgm, Mask = 00000000
598 1759239995789 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B TransferInfo: Start = 1d03f000, End = 1d03f7ff, Buffer Length = 2048, Type = Pgm, Mask = 00000000
598 1759239995789 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B TransferInfo: Start = 1fc00bf0, End = 1fc00bff, Buffer Length = 16, Type = Cfg, Mask = 00000000
598 1759239995789 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B TransferInfo: Start = 1fc00000, End = 1fc007ff, Buffer Length = 2048, Type = BootFlash, Mask = 00000000
598 1759239995789 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload End
598 1759239995789 XXXX 1759239995789, Thread 598: XXXX 1759239995789, Entering Thread 598: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
598 1759239995789 XXXX 1759239995789, Thread 598: XXXX 1759239995789, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995789 XXXX 1759239995789, Thread 598: XXXX 1759239995789, Entering Thread 598: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
598 1759239995791 XXXX 1759239995791, Thread 598: XXXX 1759239995791, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995792 XXXX 1759239995792, Thread 598: XXXX 1759239995792, Entering Thread 598: Commands::runScriptBasic, script name = SetupSerialMode, timeOut = -1 ms  
598 1759239995793 XXXX 1759239995793, Thread 598: XXXX 1759239995793, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995793 XXXX 1759239995793, Thread 598: XXXX 1759239995793, Entering Thread 598: Commands::runScriptBasic, script name = LoadLoader, timeOut = -1 ms  
598 1759239995818 XXXX 1759239995818, Thread 598: XXXX 1759239995818, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995818 XXXX 1759239995818, Thread 598: XXXX 1759239995818, Entering Thread 598: Commands::runScriptWithDownload, script name = DownloadPE  
598 1759239995848 XXXX 1759239995848, Thread 598: XXXX 1759239995848, Exiting Thread 598: Commands::runScriptWithDownload(DownloadPE)  
598 1759239995848 XXXX 1759239995848, Thread 598: XXXX 1759239995848, Entering Thread 598: Commands::runScriptBasic, script name = TestPEConnect, timeOut = -1 ms  
598 1759239995850 XXXX 1759239995850, Thread 598: XXXX 1759239995850, Exiting Thread 598: Commands::runScriptBasic  
598 1759239995850 XXXX 1759239995850, Thread 598: XXXX 1759239995850, Entering Thread 598: Commands::runScriptWithDownload, script name = WriteProgmemPE  
598 1759239997257 XXXX 1759239997257, Thread 598: XXXX 1759239997257, Exiting Thread 598: Commands::runScriptWithDownload(WriteProgmemPE)  
598 1759239997257 XXXX 1759239997257, Thread 598: XXXX 1759239997257, Entering Thread 598: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
598 1759239997716 XXXX 1759239997716, Thread 598: XXXX 1759239997716, Exiting Thread 598: Commands::runScriptBasic  
598 1759239997719 XXXX 1759239997719, Thread 598: XXXX 1759239997719, Entering Thread 598: Commands::runScriptWithDownload, script name = WriteProgmemPE  
598 1759239997758 XXXX 1759239997758, Thread 598: XXXX 1759239997758, Exiting Thread 598: Commands::runScriptWithDownload(WriteProgmemPE)  
598 1759239997758 XXXX 1759239997758, Thread 598: XXXX 1759239997758, Entering Thread 598: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
598 1759239997777 XXXX 1759239997777, Thread 598: XXXX 1759239997777, Exiting Thread 598: Commands::runScriptBasic  
598 1759239997777 XXXX 1759239997777, Thread 598: XXXX 1759239997777, Entering Thread 598: Commands::runScriptWithDownload, script name = WriteConfigmemPE  
598 1759239997780 XXXX 1759239997780, Thread 598: XXXX 1759239997780, Exiting Thread 598: Commands::runScriptWithDownload(WriteConfigmemPE)  
598 1759239997780 XXXX 1759239997780, Thread 598: XXXX 1759239997780, Entering Thread 598: Commands::runScriptWithUpload, script name = ReadProgmemPE  
598 1759239997780 XXXX 1759239997780, Thread 598: XXXX 1759239997780, Entering Thread 598: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x10 bytes long  
598 1759239997783 XXXX 1759239997783, Thread 598: XXXX 1759239997783, Exiting Thread 598: ToolCommUsb::readTransfer,  cr.status = 0x0  
598 1759239997783 XXXX 1759239997783, Thread 598: XXXX 1759239997783, Exiting Thread 598: Commands::runScriptWithUpload  
598 1759239997783 XXXX 1759239997783, Thread 598: XXXX 1759239997783, Entering Thread 598: Commands::runScriptWithDownload, script name = WriteProgmemPE  
598 1759239997821 XXXX 1759239997821, Thread 598: XXXX 1759239997821, Exiting Thread 598: Commands::runScriptWithDownload(WriteProgmemPE)  
598 1759239997821 XXXX 1759239997821, Thread 598: XXXX 1759239997821, Entering Thread 598: Commands::runScriptWithUpload, script name = ReadProgmemPE  
598 1759239997821 XXXX 1759239997821, Thread 598: XXXX 1759239997821, Entering Thread 598: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x800 bytes long  
598 1759239997856 XXXX 1759239997856, Thread 598: XXXX 1759239997856, Exiting Thread 598: ToolCommUsb::readTransfer,  cr.status = 0x0  
598 1759239997856 XXXX 1759239997856, Thread 598: XXXX 1759239997856, Exiting Thread 598: Commands::runScriptWithUpload  
598 1759239997856 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Post:SendOperation
598 1759239997856 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return Value
598 1759239997856 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B None
598 1759239997856 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return End

598 1759239997857 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Pre:endOfOperations
598 1759239997857 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload
598 1759239997857 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B null
598 1759239997857 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload End
598 1759239997857 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Post:endOfOperations
598 1759239997857 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return Value
598 1759239997857 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B None
598 1759239997857 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return End

598 1759239997860 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Pre:SendOperation
598 1759239997860 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload
598 1759239997860 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B OperationInfo: Values:
598 1759239997860 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B OperationInfo: Type = releasefromreset, Mask = 00000000, Erase = false, Production Mode = true
598 1759239997860 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload End
598 1759239997860 XXXX 1759239997860, Thread 598: XXXX 1759239997860, Entering Thread 598: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
598 1759239997861 XXXX 1759239997861, Thread 598: XXXX 1759239997861, Exiting Thread 598: Commands::runScriptBasic  
598 1759239997861 XXXX 1759239997861, Thread 598: XXXX 1759239997861, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0x42, ...  
598 1759239997862 XXXX 1759239997862, Thread 598: XXXX 1759239997862, Exiting Thread 598: Commands::runScriptBasic  
598 1759239997862 XXXX 1759239997862, Thread 598: XXXX 1759239997862, Entering Thread 598: Commands::runScriptBasic with script contents. contents[0] = 0xef, ...  
598 1759239997873 XXXX 1759239997873, Thread 598: XXXX 1759239997873, Exiting Thread 598: Commands::runScriptBasic  
598 1759239997873 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Post:SendOperation
598 1759239997873 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return Value
598 1759239997873 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B None
598 1759239997873 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return End
598 1759239997874 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is null

598 1759239997874 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:GetFirmwareInfo
598 1759239997874 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
598 1759239997874 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B null
598 1759239997874 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
598 1759239997882 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:GetFirmwareInfo
598 1759239997882 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
598 1759239997882 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: Values:
598 1759239997882 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
598 1759239997882 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End
598 1759239997882 GEN4_CONNECT_DIAGNOSTICS:Removing plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@4dcd7401
598 1759239997882 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
598 1759239997882 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
598 1759239997932 GEN4_CONNECT_DIAGNOSTICS:Calling RIDbgToolCom.Disconnect
598 1759239997932 GEN4_CONNECT_DIAGNOSTICS:Calling MPLABCommTool.Detach to remove tool from plug and play list
598 1759239997932 GEN4_CONNECT_DIAGNOSTICS:Calling RIDbgToolCom.DisconnectFromMPlabComm
598 1759239997932 GEN4_CONNECT_DIAGNOSTICS:Calling MPLABCommTool.Disconnect
638 1759240132919 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is NOT null
638 1759240132919 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9012, AttachedToolVID = 4d8
638 1759240132919 GEN4_CONNECT_DIAGNOSTICS:transport type = USB
638 1759240132919 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9012, AttachedToolVID = 4d8
638 1759240132923 com.microchip.mplab.mdbcore.RealICETool.RIDbgToolCom
638 1759240132923 GEN4_CONNECT_DIAGNOSTICS:Before MPLABCommTool.Connect()
638 1759240132923 GEN4_CONNECT_DIAGNOSTICS:After MPLABCommTool.Connect()
638 1759240132923 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool.Connect() returned MPLABCOMM_NO_ERROR
638 1759240132923 GEN4_CONNECT_DIAGNOSTICS:Attaching to MPLABCommTool plugnplay
638 1759240132923 GEN4_CONNECT_DIAGNOSTICS:Adding new plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@50580ec9
638 1759240132923 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
638 1759240132923 GEN4_CONNECT_DIAGNOSTICS:com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@50580ec9
638 1759240132923 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
638 1759240132923 GEN4_CONNECT_DIAGNOSTICS:Registering for alternate PNP notifications. CommPnPCriteria.cPIDList = [2177, 2179, 217a, 2141, 9017, 901b, 9036, 9035], CommPnPCriteria.cSerialNumber = bur213375184

638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:init
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: Values:
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: pcAddress = 7fffffffffffffff, Vpp = 3.30, useRowEraseIfVoltageIsLow = false, voltageBelowWhichUseRowErase = 0.00, deviceName = PIC32MX270F256B, programmerType = PIC32MX_JTAG_ONLY
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: MemInfo values:
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = ffffffff, exists = true, startAddr = 1d000000, endAddr = 1d03ffff, rowSize = 0400, rowEraseSize = 0400, addrInc = 0004, widthProgram = 0004
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = ffffffff, exists = true, startAddr = 1fc00bf0, endAddr = 1fc00bff, rowSize = 0001, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = true, startAddr = 00000000, endAddr = 00000000, rowSize = 0400, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0400, addrInc = 0000, widthProgram = 0000
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = ffffffff, exists = true, startAddr = 1f800000, endAddr = 1f886fff, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 7fffffff, exists = true, startAddr = ffffffff, endAddr = fffffffe, rowSize = 0001, rowEraseSize = 0000, addrInc = 0001, widthProgram = 0001
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132948 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B DeviceInfo: CfgRequiredBitsMask Values:
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Address = 1fc00bf0, Mask = f000ffff
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Address = 1fc00bf4, Mask = 00078777
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Address = 1fc00bf8, Mask = 03dff7a7
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Address = 1fc00bfc, Mask = 1107fc1c
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B BasicInfo: Values:
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B BasicInfo: InputStream = com.microchip.mplab.libs.toolpacksupport.EquatableFileInputStream@1fa17626, ToolFlavor = PICKit4
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:init
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B none
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B RI4DebugInterface
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.RI4ToolsController.implementations.RI4DebugInterfaceImpl@7ac1ede6
638 1759240132949 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B RI4ProgramInterface
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ProgramInterfaceImpl@44a85222
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B RI4ConnectInterface
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.PK4ToolsController.PK4ConnectInterfaceImpl@54163238
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End
638 1759240132950 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]
638 1759240132950 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
638 1759240132950 GEN4_CONNECT_DIAGNOSTICS:Setting selected tool type to pk4
638 1759240132950 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
638 1759240132950 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]

638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B RI4ControllerDiagnosticsInterface
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ControllerDiagnosticsInterfaceImpl@3dcd61fc
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B ProgrammerToGo
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B com.microchip.mplab.libs.RI4ToolsController.implementations.ProgrammerToGoImpl@4816057e
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Pre:GetInterfaceProvider
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Status
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Payload End
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Post:GetInterfaceProvider
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return Value
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B null
638 1759240132950 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX270F256B Return End

638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Pre:SetProgramExec
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B FileRegs
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B a0000900
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Length = 1688
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Payload End
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Post:SetProgramExec
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return Value
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B true
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX270F256B Return End
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@4e29671c
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:uMode = checkingVersions
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:Parsing file  for firmware updates
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ParseSelectedVersionsFromJamFile()
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:Jame file line = boot.hex,010000
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:Jame file line = scripts.xml,000671
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app1 020135, 0040C000
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app2 1.15.20, 00500000
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app3 000000, FFFFFFFF
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app4 000000, FFFFFFFF
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app5 000000, FFFFFFFF
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app6 000000, FFFFFFFF
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app7 000000, FFFFFFFF
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app8 000000, FFFFFFFF
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ri4ParseSelectedVersionsFromJamFile()
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
638 1759240132958 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4

638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:EstablishCommunincations
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B com.microchip.mplab.mdbcore.PK4Tool.PK4Com@18d4107
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:EstablishCommunincations
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B true
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:GetFirmwareInfo
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B null
638 1759240132958 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
638 1759240132966 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:GetFirmwareInfo
638 1759240132966 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
638 1759240132966 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: Values:
638 1759240132966 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
638 1759240132966 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End
638 1759240132973 GEN4_CONNECT_DIAGNOSTICS:appNeedsUpdate returned false
638 1759240132973 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

638 1759240132973 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:EstablishCommunincations
638 1759240132973 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
638 1759240132973 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B com.microchip.mplab.mdbcore.PK4Tool.PK4Com@18d4107
638 1759240132973 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
638 1759240132974 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:EstablishCommunincations
638 1759240132974 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
638 1759240132974 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B true
638 1759240132974 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

638 1759240132974 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:GetFirmwareInfo
638 1759240132974 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
638 1759240132974 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B null
638 1759240132974 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
638 1759240132982 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:GetFirmwareInfo
638 1759240132982 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
638 1759240132982 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: Values:
638 1759240132982 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
638 1759240132982 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

638 1759240132982 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:GetFirmwareInfo
638 1759240132982 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
638 1759240132982 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B null
638 1759240132982 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
638 1759240132989 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:GetFirmwareInfo
638 1759240132989 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
638 1759240132989 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: Values:
638 1759240132989 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
638 1759240132989 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End
638 1759240132989 XXXX 1759240132989, Thread 638: XXXX 1759240132989, Entering Thread 638: Commands::runScriptWithUpload with script contents. contents[0] = 0x5e, ...  
638 1759240132989 XXXX 1759240132989, Thread 638: XXXX 1759240132989, Entering Thread 638: ToolCommUsb::readTransfer, sideData is 0xd bytes long, transferDataLength is 0x4 bytes long  
638 1759240132990 XXXX 1759240132990, Thread 638: XXXX 1759240132990, Exiting Thread 638: ToolCommUsb::readTransfer,  cr.status = 0x0  
638 1759240132990 XXXX 1759240132990, Thread 638: XXXX 1759240132990, Exiting Thread 638: Commands::runScriptWithUpload  
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@4e29671c
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:uMode = done
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:Don't upgrade fimware = false
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
638 1759240132990 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

638 1759240132990 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:SetPowerInfo
638 1759240132990 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
638 1759240132990 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B PowerInfo: Values:
638 1759240132991 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B PowerInfo: shotDownSystem = false, isToolPower = true, voltage = 3.250000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
638 1759240132991 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
638 1759240132991 XXXX 1759240132991, Thread 638: XXXX 1759240132991, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
638 1759240132991 XXXX 1759240132991, Thread 638: XXXX 1759240132991, Exiting Thread 638: Commands::runScriptBasic  
638 1759240132991 XXXX 1759240132991, Thread 638: XXXX 1759240132991, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
638 1759240132992 XXXX 1759240132992, Thread 638: XXXX 1759240132992, Exiting Thread 638: Commands::runScriptBasic  
638 1759240132992 XXXX 1759240132992, Thread 638: XXXX 1759240132992, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
638 1759240133005 XXXX 1759240133005, Thread 638: XXXX 1759240133005, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133005 XXXX 1759240133005, Thread 638: XXXX 1759240133005, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
638 1759240133182 XXXX 1759240133182, Thread 638: XXXX 1759240133182, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133182 XXXX 1759240133182, Thread 638: XXXX 1759240133182, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
638 1759240133187 XXXX 1759240133187, Thread 638: XXXX 1759240133187, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133187 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:SetPowerInfo
638 1759240133187 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
638 1759240133187 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B none
638 1759240133187 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

638 1759240133187 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:SetLEDBrightness
638 1759240133187 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
638 1759240133187 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B 5
638 1759240133187 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
638 1759240133187 XXXX 1759240133187, Thread 638: XXXX 1759240133187, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xcf, ...  
638 1759240133188 XXXX 1759240133188, Thread 638: XXXX 1759240133188, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133188 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:SetLEDBrightness
638 1759240133188 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
638 1759240133188 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B none
638 1759240133188 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

638 1759240133188 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:SetToolInfo
638 1759240133188 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
638 1759240133188 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B ToolInfo: Values:
638 1759240133188 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B ToolInfo: speedLevel = 1, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
638 1759240133188 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
638 1759240133188 XXXX 1759240133188, Thread 638: XXXX 1759240133188, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
638 1759240133188 XXXX 1759240133188, Thread 638: XXXX 1759240133188, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133188 XXXX 1759240133188, Thread 638: XXXX 1759240133188, Entering Thread 638: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
638 1759240133190 XXXX 1759240133190, Thread 638: XXXX 1759240133190, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133190 XXXX 1759240133190, Thread 638: XXXX 1759240133190, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
638 1759240133191 XXXX 1759240133191, Thread 638: XXXX 1759240133191, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133191 XXXX 1759240133191, Thread 638: XXXX 1759240133191, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xec, ...  
638 1759240133192 XXXX 1759240133192, Thread 638: XXXX 1759240133192, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133192 XXXX 1759240133192, Thread 638: XXXX 1759240133192, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
638 1759240133193 XXXX 1759240133193, Thread 638: XXXX 1759240133193, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133193 XXXX 1759240133193, Thread 638: XXXX 1759240133193, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
638 1759240133194 XXXX 1759240133194, Thread 638: XXXX 1759240133194, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133194 XXXX 1759240133194, Thread 638: XXXX 1759240133194, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
638 1759240133195 XXXX 1759240133195, Thread 638: XXXX 1759240133195, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133195 XXXX 1759240133195, Thread 638: XXXX 1759240133195, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
638 1759240133196 XXXX 1759240133196, Thread 638: XXXX 1759240133196, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133196 XXXX 1759240133196, Thread 638: XXXX 1759240133196, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
638 1759240133197 XXXX 1759240133197, Thread 638: XXXX 1759240133197, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133197 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Post:SetToolInfo
638 1759240133197 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return Value
638 1759240133197 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B none
638 1759240133197 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Return End

638 1759240133198 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Pre:GetTargetIDInfo
638 1759240133198 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload
638 1759240133198 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B null
638 1759240133198 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX270F256B Payload End
638 1759240133199 XXXX 1759240133199, Thread 638: XXXX 1759240133199, Entering Thread 638: Commands::runScriptBasic, script name = ReadDeviceParameters, timeOut = -1 ms  
638 1759240133200 XXXX 1759240133200, Thread 638: XXXX 1759240133200, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133200 XXXX 1759240133200, Thread 638: XXXX 1759240133200, Entering Thread 638: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
638 1759240133207 XXXX 1759240133207, Thread 638: XXXX 1759240133207, Exiting Thread 638: Commands::runScriptBasic  
638 1759240133207 XXXX 1759240133207, Thread 638: XXXX 1759240133207, Entering Thread 638: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
638 1759240135255 XXXX 1759240135255, Thread 638: Type = runScript, Script name = InitJTAG, Status = 0x104
 
