384 1683082439040 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is NOT null
384 1683082439040 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9012, AttachedToolVID = 4d8
384 1683082439040 GEN4_CONNECT_DIAGNOSTICS:transport type = USB
384 1683082439041 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9012, AttachedToolVID = 4d8
384 1683082441093 GEN4_CONNECT_DIAGNOSTICS:Before MPLABCommTool.Connect()
384 1683082441093 GEN4_CONNECT_DIAGNOSTICS:After MPLABCommTool.Connect()
384 1683082441093 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool.Connect() returned MPLABCOMM_NO_ERROR
384 1683082441093 GEN4_CONNECT_DIAGNOSTICS:Attaching to MPLABCommTool plugnplay
384 1683082441101 GEN4_CONNECT_DIAGNOSTICS:Adding new plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@76eac767
384 1683082441101 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
384 1683082441101 GEN4_CONNECT_DIAGNOSTICS:com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@76eac767
384 1683082441101 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
384 1683082441103 GEN4_CONNECT_DIAGNOSTICS:Registering for alternate PNP notifications. CommPnPCriteria.cPIDList = [2177, 2179, 217a, 2141, 9017, 901b, 9036, 9035], CommPnPCriteria.cSerialNumber = bur213375184

384 1683082441448 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:init
384 1683082441448 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: Values:
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: pcAddress = 7fffffffffffffff, Vpp = 3.30, useRowEraseIfVoltageIsLow = false, voltageBelowWhichUseRowErase = 0.00, deviceName = PIC32MX695F512H, programmerType = PIC32MX_SSM
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: MemInfo values:
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = ffffffff, exists = true, startAddr = 1d000000, endAddr = 1d07ffff, rowSize = 1000, rowEraseSize = 1000, addrInc = 0004, widthProgram = 0004
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = ffffffff, exists = true, startAddr = 1fc02ff0, endAddr = 1fc02fff, rowSize = 0001, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = true, startAddr = 00000000, endAddr = 00000000, rowSize = 1000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 1000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = ffffffff, exists = true, startAddr = 1f800000, endAddr = 1f88cfff, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 7fffffff, exists = true, startAddr = ffffffff, endAddr = fffffffe, rowSize = 0001, rowEraseSize = 0000, addrInc = 0001, widthProgram = 0001
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
384 1683082441449 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: CfgRequiredBitsMask Values:
384 1683082441450 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ff0, Mask = c307ffff
384 1683082441450 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ff4, Mask = 00078777
384 1683082441450 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ff8, Mask = 009ff7a7
384 1683082441450 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ffc, Mask = 110ff00c
384 1683082441450 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H BasicInfo: Values:
384 1683082441450 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H BasicInfo: InputStream = com.microchip.mplab.libs.toolpacksupport.EquatableFileInputStream@1963d89, ToolFlavor = PICKit4
384 1683082441450 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443207 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:init
384 1683082443207 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443207 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H none
384 1683082443207 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

384 1683082443207 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
384 1683082443207 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
384 1683082443207 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4DebugInterface
384 1683082443207 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443207 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
384 1683082443207 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443207 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4DebugInterfaceImpl@3aa9c3eb
384 1683082443207 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

384 1683082443225 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
384 1683082443225 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
384 1683082443225 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ProgramInterface
384 1683082443225 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443225 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
384 1683082443225 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443225 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ProgramInterfaceImpl@114c3d76
384 1683082443225 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

384 1683082443239 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
384 1683082443239 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
384 1683082443239 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ConnectInterface
384 1683082443239 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443242 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
384 1683082443242 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443242 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.PK4ToolsController.PK4ConnectInterfaceImpl@64be927e
384 1683082443242 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End
384 1683082443248 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]
384 1683082443248 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
384 1683082443248 GEN4_CONNECT_DIAGNOSTICS:Setting selected tool type to pk4
384 1683082443248 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
384 1683082443248 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]

384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:selectCore
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PIC32MX695F512H
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:selectCore
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ControllerDiagnosticsInterface
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ControllerDiagnosticsInterfaceImpl@3aaedfd3
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H ProgrammerToGo
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.ProgrammerToGoImpl@241f592
384 1683082443250 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

384 1683082443251 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
384 1683082443251 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
384 1683082443251 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Status
384 1683082443251 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443251 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
384 1683082443251 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443251 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H null
384 1683082443251 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

384 1683082443257 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SetProgramExec
384 1683082443257 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
384 1683082443259 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H FileRegs
384 1683082443259 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H a0000900
384 1683082443259 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Length = 4176
384 1683082443259 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
384 1683082443259 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SetProgramExec
384 1683082443259 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
384 1683082443259 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H true
384 1683082443259 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End
384 1683082443259 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
384 1683082443259 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@18e95633
384 1683082443259 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
384 1683082443264 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
384 1683082443264 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
384 1683082443264 GEN4_CONNECT_DIAGNOSTICS:uMode = checkingVersions
384 1683082443264 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
384 1683082443264 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
384 1683082443264 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
384 1683082443264 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.GetUpdateInfo()
384 1683082443265 GEN4_CONNECT_DIAGNOSTICS:Parsing file  for firmware updates
384 1683082443265 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.ParseSelectedVersionsFromJamFile()
384 1683082443265 GEN4_CONNECT_DIAGNOSTICS:Jame file line = boot.hex,010000
384 1683082443265 GEN4_CONNECT_DIAGNOSTICS:Jame file line = scripts.xml,000535
384 1683082443265 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app1 000854, 0040C000
384 1683082443265 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app2 1.14.268, 00500000
384 1683082443265 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app3 000000, FFFFFFFF
384 1683082443265 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app4 000000, FFFFFFFF
384 1683082443265 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app5 000000, FFFFFFFF
384 1683082443265 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app6 000000, FFFFFFFF
384 1683082443265 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app7 000000, FFFFFFFF
384 1683082443265 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app8 000000, FFFFFFFF
384 1683082443266 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.ri4ParseSelectedVersionsFromJamFile()
384 1683082443266 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.GetUpdateInfo()
384 1683082443266 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4

384 1683082443266 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
384 1683082443266 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
384 1683082443266 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@39591ca7
384 1683082443266 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443271 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
384 1683082443271 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443271 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
384 1683082443271 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

384 1683082443271 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
384 1683082443271 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
384 1683082443271 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
384 1683082443271 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443301 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
384 1683082443301 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443301 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
384 1683082443301 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 00.08.54, fpgaVer = ff.ff.ff, scriptVer = 00.05.35, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 86fedc5c2e, PCB_ID = 4
384 1683082443301 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
384 1683082443308 GEN4_CONNECT_DIAGNOSTICS:appNeedsUpdate returned false
384 1683082443308 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

384 1683082443308 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
384 1683082443308 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
384 1683082443308 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@39591ca7
384 1683082443308 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443308 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
384 1683082443308 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443308 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
384 1683082443308 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

384 1683082443309 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
384 1683082443309 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
384 1683082443309 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
384 1683082443309 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
384 1683082443337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
384 1683082443337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 00.08.54, fpgaVer = ff.ff.ff, scriptVer = 00.05.35, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 86fedc5c2e, PCB_ID = 4
384 1683082443337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
384 1683082443340 XXXX 1683082443340, Thread 384: XXXX 1683082443340, Entering Thread 384: Commands::runScriptWithUpload with script contents. contents[0] = 0x5e, ...  
384 1683082443341 XXXX 1683082443341, Thread 384: XXXX 1683082443341, Entering Thread 384: ToolCommUsb::readTransfer, sideData is 0xd bytes long, transferDataLength is 0x4 bytes long  
384 1683082443344 XXXX 1683082443344, Thread 384: XXXX 1683082443344, Exiting Thread 384: ToolCommUsb::readTransfer,  cr.status = 0x0  
384 1683082443344 XXXX 1683082443344, Thread 384: XXXX 1683082443344, Exiting Thread 384: Commands::runScriptWithUpload  
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@18e95633
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:uMode = done
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.updatePk4HybridFirmware()
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:Don't upgrade fimware = false
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.updatePk4HybridFirmware()
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
384 1683082443344 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

384 1683082443345 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetPowerInfo
384 1683082443345 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
384 1683082443345 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: Values:
384 1683082443345 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: shotDownSystem = false, isToolPower = true, voltage = 3.250000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
384 1683082443345 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443345 XXXX 1683082443345, Thread 384: XXXX 1683082443345, Entering Thread 384: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
384 1683082443346 XXXX 1683082443346, Thread 384: XXXX 1683082443346, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443346 XXXX 1683082443346, Thread 384: XXXX 1683082443346, Entering Thread 384: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
384 1683082443360 XXXX 1683082443360, Thread 384: XXXX 1683082443360, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443360 XXXX 1683082443360, Thread 384: XXXX 1683082443360, Entering Thread 384: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
384 1683082443538 XXXX 1683082443538, Thread 384: XXXX 1683082443538, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443538 XXXX 1683082443538, Thread 384: XXXX 1683082443538, Entering Thread 384: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
384 1683082443547 XXXX 1683082443547, Thread 384: XXXX 1683082443547, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443548 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetPowerInfo
384 1683082443548 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443548 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
384 1683082443548 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

384 1683082443548 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetLEDBrightness
384 1683082443548 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
384 1683082443548 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H 5
384 1683082443548 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443548 XXXX 1683082443548, Thread 384: XXXX 1683082443548, Entering Thread 384: Commands::runScriptBasic with script contents. contents[0] = 0xcf, ...  
384 1683082443551 XXXX 1683082443551, Thread 384: XXXX 1683082443551, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443551 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetLEDBrightness
384 1683082443551 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443551 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
384 1683082443551 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

384 1683082443551 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetToolInfo
384 1683082443551 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
384 1683082443551 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: Values:
384 1683082443551 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: speedLevel = 1, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
384 1683082443551 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443551 XXXX 1683082443551, Thread 384: XXXX 1683082443551, Entering Thread 384: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
384 1683082443552 XXXX 1683082443552, Thread 384: XXXX 1683082443552, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443552 XXXX 1683082443552, Thread 384: XXXX 1683082443552, Entering Thread 384: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
384 1683082443553 XXXX 1683082443553, Thread 384: XXXX 1683082443553, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443553 XXXX 1683082443553, Thread 384: XXXX 1683082443553, Entering Thread 384: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
384 1683082443554 XXXX 1683082443554, Thread 384: XXXX 1683082443554, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443554 XXXX 1683082443554, Thread 384: XXXX 1683082443554, Entering Thread 384: Commands::runScriptBasic with script contents. contents[0] = 0xec, ...  
384 1683082443555 XXXX 1683082443555, Thread 384: XXXX 1683082443555, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443555 XXXX 1683082443555, Thread 384: XXXX 1683082443555, Entering Thread 384: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
384 1683082443556 XXXX 1683082443556, Thread 384: XXXX 1683082443556, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443556 XXXX 1683082443556, Thread 384: XXXX 1683082443556, Entering Thread 384: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
384 1683082443557 XXXX 1683082443557, Thread 384: XXXX 1683082443557, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443557 XXXX 1683082443557, Thread 384: XXXX 1683082443557, Entering Thread 384: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
384 1683082443559 XXXX 1683082443559, Thread 384: XXXX 1683082443559, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443559 XXXX 1683082443559, Thread 384: XXXX 1683082443559, Entering Thread 384: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
384 1683082443560 XXXX 1683082443560, Thread 384: XXXX 1683082443560, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443560 XXXX 1683082443560, Thread 384: XXXX 1683082443560, Entering Thread 384: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
384 1683082443562 XXXX 1683082443562, Thread 384: XXXX 1683082443562, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443562 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetToolInfo
384 1683082443562 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
384 1683082443562 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
384 1683082443562 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

384 1683082443563 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetTargetIDInfo
384 1683082443563 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
384 1683082443563 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
384 1683082443563 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
384 1683082443565 XXXX 1683082443565, Thread 384: XXXX 1683082443565, Entering Thread 384: Commands::runScriptBasic, script name = ReadDeviceParameters, timeOut = -1 ms  
384 1683082443566 XXXX 1683082443566, Thread 384: XXXX 1683082443566, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443566 XXXX 1683082443566, Thread 384: XXXX 1683082443566, Entering Thread 384: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
384 1683082443572 XXXX 1683082443572, Thread 384: XXXX 1683082443572, Exiting Thread 384: Commands::runScriptBasic  
384 1683082443572 XXXX 1683082443572, Thread 384: XXXX 1683082443572, Entering Thread 384: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
384 1683082444086 XXXX 1683082444086, Thread 384: Type = runScript, Script name = InitJTAG, Status = 0x104
 
