638 1697709909394 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
638 1697709909394 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
638 1697709909394 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.00.85, fpgaVer = ff.ff.ff, scriptVer = 00.05.85, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = d33d758f73, PCB_ID = 4
638 1697709909394 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
638 1697709909394 XXXX 1697709909394, Thread 638: XXXX 1697709909394, Entering Thread 638: Commands::runScriptWithUpload with script contents. contents[0] = 0x5e, ...  
638 1697709909394 XXXX 1697709909394, Thread 638: XXXX 1697709909394, Entering Thread 638: ToolCommUsb::readTransfer, sideData is 0xd bytes long, transferDataLength is 0x4 bytes long  
638 1697709909396 XXXX 1697709909396, Thread 638: XXXX 1697709909396, Exiting Thread 638: ToolCommUsb::readTransfer,  cr.status = 0x0  
638 1697709909396 XXXX 1697709909396, Thread 638: XXXX 1697709909396, Exiting Thread 638: Commands::runScriptWithUpload  

638 1697709909396 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetPowerInfo
638 1697709909396 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
638 1697709909396 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: Values:
638 1697709909396 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: shotDownSystem = false, isToolPower = true, voltage = 3.250000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
638 1697709909396 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
638 1697709909396 XXXX 1697709909396, Thread 638: XXXX 1697709909396, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
638 1697709909397 XXXX 1697709909397, Thread 638: XXXX 1697709909397, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909397 XXXX 1697709909397, Thread 638: XXXX 1697709909397, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
638 1697709909398 XXXX 1697709909398, Thread 638: XXXX 1697709909398, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909398 XXXX 1697709909398, Thread 638: XXXX 1697709909398, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
638 1697709909410 XXXX 1697709909410, Thread 638: XXXX 1697709909410, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909410 XXXX 1697709909410, Thread 638: XXXX 1697709909410, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
638 1697709909586 XXXX 1697709909586, Thread 638: XXXX 1697709909586, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909586 XXXX 1697709909586, Thread 638: XXXX 1697709909586, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
638 1697709909592 XXXX 1697709909592, Thread 638: XXXX 1697709909592, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909592 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetPowerInfo
638 1697709909592 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
638 1697709909592 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
638 1697709909592 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

638 1697709909592 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetLEDBrightness
638 1697709909592 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
638 1697709909592 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H 5
638 1697709909592 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
638 1697709909592 XXXX 1697709909592, Thread 638: XXXX 1697709909592, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xcf, ...  
638 1697709909593 XXXX 1697709909593, Thread 638: XXXX 1697709909593, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909593 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetLEDBrightness
638 1697709909593 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
638 1697709909593 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
638 1697709909593 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

638 1697709909593 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetToolInfo
638 1697709909593 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
638 1697709909593 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: Values:
638 1697709909593 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: speedLevel = 1, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
638 1697709909593 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
638 1697709909593 XXXX 1697709909593, Thread 638: XXXX 1697709909593, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
638 1697709909593 XXXX 1697709909593, Thread 638: XXXX 1697709909593, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909593 XXXX 1697709909593, Thread 638: XXXX 1697709909593, Entering Thread 638: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
638 1697709909594 XXXX 1697709909594, Thread 638: XXXX 1697709909594, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909594 XXXX 1697709909594, Thread 638: XXXX 1697709909594, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
638 1697709909595 XXXX 1697709909595, Thread 638: XXXX 1697709909595, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909595 XXXX 1697709909595, Thread 638: XXXX 1697709909595, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xec, ...  
638 1697709909596 XXXX 1697709909596, Thread 638: XXXX 1697709909596, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909596 XXXX 1697709909596, Thread 638: XXXX 1697709909596, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
638 1697709909597 XXXX 1697709909597, Thread 638: XXXX 1697709909597, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909597 XXXX 1697709909597, Thread 638: XXXX 1697709909597, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
638 1697709909598 XXXX 1697709909598, Thread 638: XXXX 1697709909598, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909598 XXXX 1697709909598, Thread 638: XXXX 1697709909598, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
638 1697709909600 XXXX 1697709909600, Thread 638: XXXX 1697709909600, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909600 XXXX 1697709909600, Thread 638: XXXX 1697709909600, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
638 1697709909600 XXXX 1697709909600, Thread 638: XXXX 1697709909600, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909600 XXXX 1697709909600, Thread 638: XXXX 1697709909600, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
638 1697709909602 XXXX 1697709909602, Thread 638: XXXX 1697709909602, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909602 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetToolInfo
638 1697709909602 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
638 1697709909602 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
638 1697709909602 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

638 1697709909607 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
638 1697709909607 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
638 1697709909607 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
638 1697709909607 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = erase, Mask = 00000000, Erase = false, Production Mode = true
638 1697709909607 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 0, Type = Pgm, Mask = 00000000
638 1697709909607 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 0, Type = Cfg, Mask = 00000000
638 1697709909607 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc02fef, Buffer Length = 0, Type = BootFlash, Mask = 00000000
638 1697709909607 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
638 1697709909607 XXXX 1697709909607, Thread 638: XXXX 1697709909607, Entering Thread 638: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
638 1697709909614 XXXX 1697709909614, Thread 638: XXXX 1697709909614, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909614 XXXX 1697709909614, Thread 638: XXXX 1697709909614, Entering Thread 638: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
638 1697709909614 XXXX 1697709909614, Thread 638: XXXX 1697709909614, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909614 XXXX 1697709909614, Thread 638: XXXX 1697709909614, Entering Thread 638: Commands::runScriptBasic, script name = EraseChip, timeOut = 30000 ms  
638 1697709909716 XXXX 1697709909716, Thread 638: XXXX 1697709909716, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909716 XXXX 1697709909716, Thread 638: XXXX 1697709909716, Entering Thread 638: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
638 1697709909718 XXXX 1697709909718, Thread 638: XXXX 1697709909718, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909718 XXXX 1697709909718, Thread 638: XXXX 1697709909718, Entering Thread 638: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
638 1697709909725 XXXX 1697709909725, Thread 638: XXXX 1697709909725, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909725 XXXX 1697709909725, Thread 638: XXXX 1697709909725, Entering Thread 638: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
638 1697709909725 XXXX 1697709909725, Thread 638: XXXX 1697709909725, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909725 XXXX 1697709909725, Thread 638: XXXX 1697709909725, Entering Thread 638: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
638 1697709909726 XXXX 1697709909726, Thread 638: XXXX 1697709909726, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909726 XXXX 1697709909726, Thread 638: XXXX 1697709909726, Entering Thread 638: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
638 1697709909727 XXXX 1697709909727, Thread 638: XXXX 1697709909727, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909727 XXXX 1697709909727, Thread 638: XXXX 1697709909727, Entering Thread 638: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
638 1697709909728 XXXX 1697709909728, Thread 638: XXXX 1697709909728, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909728 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
638 1697709909728 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
638 1697709909728 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
638 1697709909728 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

638 1697709909731 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
638 1697709909731 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
638 1697709909731 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
638 1697709909731 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = write, Mask = 00000000, Erase = false, Production Mode = true
638 1697709909731 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 524288, Type = Pgm, Mask = 00000000
638 1697709909731 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 16, Type = Cfg, Mask = 00000000
638 1697709909731 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc01fff, Buffer Length = 8192, Type = BootFlash, Mask = 00000000
638 1697709909731 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
638 1697709909731 XXXX 1697709909731, Thread 638: XXXX 1697709909731, Entering Thread 638: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
638 1697709909731 XXXX 1697709909731, Thread 638: XXXX 1697709909731, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909731 XXXX 1697709909731, Thread 638: XXXX 1697709909731, Entering Thread 638: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
638 1697709909733 XXXX 1697709909733, Thread 638: XXXX 1697709909733, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909733 XXXX 1697709909733, Thread 638: XXXX 1697709909733, Entering Thread 638: Commands::runScriptBasic, script name = SetupSerialMode, timeOut = -1 ms  
638 1697709909734 XXXX 1697709909734, Thread 638: XXXX 1697709909734, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909734 XXXX 1697709909734, Thread 638: XXXX 1697709909734, Entering Thread 638: Commands::runScriptBasic, script name = LoadLoader, timeOut = -1 ms  
638 1697709909759 XXXX 1697709909759, Thread 638: XXXX 1697709909759, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909759 XXXX 1697709909759, Thread 638: XXXX 1697709909759, Entering Thread 638: Commands::runScriptWithDownload, script name = DownloadPE  
638 1697709909829 XXXX 1697709909829, Thread 638: XXXX 1697709909829, Exiting Thread 638: Commands::runScriptWithDownload(DownloadPE)  
638 1697709909829 XXXX 1697709909829, Thread 638: XXXX 1697709909829, Entering Thread 638: Commands::runScriptBasic, script name = TestPEConnect, timeOut = -1 ms  
638 1697709909831 XXXX 1697709909831, Thread 638: XXXX 1697709909831, Exiting Thread 638: Commands::runScriptBasic  
638 1697709909831 XXXX 1697709909831, Thread 638: XXXX 1697709909831, Entering Thread 638: Commands::runScriptWithDownload, script name = WriteProgmemPE  
638 1697709918574 XXXX 1697709918574, Thread 638: XXXX 1697709918574, Exiting Thread 638: Commands::runScriptWithDownload(WriteProgmemPE)  
638 1697709918574 XXXX 1697709918574, Thread 638: XXXX 1697709918574, Entering Thread 638: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
638 1697709918637 XXXX 1697709918637, Thread 638: XXXX 1697709918637, Exiting Thread 638: Commands::runScriptBasic  
638 1697709918637 XXXX 1697709918637, Thread 638: XXXX 1697709918637, Entering Thread 638: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
638 1697709918701 XXXX 1697709918701, Thread 638: XXXX 1697709918701, Exiting Thread 638: Commands::runScriptBasic  
638 1697709918701 XXXX 1697709918701, Thread 638: XXXX 1697709918701, Entering Thread 638: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
638 1697709918765 XXXX 1697709918765, Thread 638: XXXX 1697709918765, Exiting Thread 638: Commands::runScriptBasic  
638 1697709918765 XXXX 1697709918765, Thread 638: XXXX 1697709918765, Entering Thread 638: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
638 1697709918829 XXXX 1697709918829, Thread 638: XXXX 1697709918829, Exiting Thread 638: Commands::runScriptBasic  
638 1697709918829 XXXX 1697709918829, Thread 638: XXXX 1697709918829, Entering Thread 638: Commands::runScriptWithDownload, script name = WriteConfigmemPE  
638 1697709918832 XXXX 1697709918832, Thread 638: XXXX 1697709918832, Exiting Thread 638: Commands::runScriptWithDownload(WriteConfigmemPE)  
638 1697709918832 XXXX 1697709918832, Thread 638: XXXX 1697709918832, Entering Thread 638: Commands::runScriptWithUpload, script name = ReadProgmemPE  
638 1697709918832 XXXX 1697709918832, Thread 638: XXXX 1697709918832, Entering Thread 638: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x10 bytes long  
638 1697709918834 XXXX 1697709918834, Thread 638: XXXX 1697709918834, Exiting Thread 638: ToolCommUsb::readTransfer,  cr.status = 0x0  
638 1697709918834 XXXX 1697709918834, Thread 638: XXXX 1697709918834, Exiting Thread 638: Commands::runScriptWithUpload  
638 1697709918834 XXXX 1697709918834, Thread 638: XXXX 1697709918834, Entering Thread 638: Commands::runScriptWithDownload, script name = WriteProgmemPE  
638 1697709918976 XXXX 1697709918976, Thread 638: XXXX 1697709918976, Exiting Thread 638: Commands::runScriptWithDownload(WriteProgmemPE)  
638 1697709918976 XXXX 1697709918976, Thread 638: XXXX 1697709918976, Entering Thread 638: Commands::runScriptWithUpload, script name = ReadProgmemPE  
638 1697709918976 XXXX 1697709918976, Thread 638: XXXX 1697709918976, Entering Thread 638: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x2000 bytes long  
638 1697709919111 XXXX 1697709919111, Thread 638: XXXX 1697709919111, Exiting Thread 638: ToolCommUsb::readTransfer,  cr.status = 0x0  
638 1697709919111 XXXX 1697709919111, Thread 638: XXXX 1697709919111, Exiting Thread 638: Commands::runScriptWithUpload  
638 1697709919111 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
638 1697709919111 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
638 1697709919111 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
638 1697709919111 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

638 1697709919111 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:endOfOperations
638 1697709919111 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
638 1697709919111 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H null
638 1697709919111 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
638 1697709919111 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:endOfOperations
638 1697709919111 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
638 1697709919111 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
638 1697709919111 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

638 1697709919113 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
638 1697709919113 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
638 1697709919113 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
638 1697709919113 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = releasefromreset, Mask = 00000000, Erase = false, Production Mode = true
638 1697709919113 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
638 1697709919113 XXXX 1697709919113, Thread 638: XXXX 1697709919113, Entering Thread 638: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
638 1697709919115 XXXX 1697709919115, Thread 638: XXXX 1697709919115, Exiting Thread 638: Commands::runScriptBasic  
638 1697709919115 XXXX 1697709919115, Thread 638: XXXX 1697709919115, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0x42, ...  
638 1697709919116 XXXX 1697709919116, Thread 638: XXXX 1697709919116, Exiting Thread 638: Commands::runScriptBasic  
638 1697709919116 XXXX 1697709919116, Thread 638: XXXX 1697709919116, Entering Thread 638: Commands::runScriptBasic with script contents. contents[0] = 0xef, ...  
638 1697709919127 XXXX 1697709919127, Thread 638: XXXX 1697709919127, Exiting Thread 638: Commands::runScriptBasic  
638 1697709919127 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
638 1697709919127 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
638 1697709919127 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
638 1697709919127 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End
209 1697709931243 GEN4_CONNECT_DIAGNOSTICS:Calling Update on plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@1cc5184c
209 1697709931243 GEN4_CONNECT_DIAGNOSTICS:Entering plug and play Update(). Attached PID = 9012
209 1697709931243 GEN4_CONNECT_DIAGNOSTICS:Entering MPLABCommEvent handler
209 1697709931243 GEN4_CONNECT_DIAGNOSTICS:MPLABCommEvent.pid = 9012
209 1697709931243 GEN4_CONNECT_DIAGNOSTICS:eventType = MPLABCOMM_TOOL_UNPLUGGED
209 1697709931243 GEN4_CONNECT_DIAGNOSTICS:Exiting plug and play Update()
209 1697710031325 GEN4_CONNECT_DIAGNOSTICS:Before MPLABCommTool.Connect()
209 1697710031325 GEN4_CONNECT_DIAGNOSTICS:After MPLABCommTool.Connect()
209 1697710031325 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool.Connect() returned MPLABCOMM_NO_ERROR
209 1697710031325 GEN4_CONNECT_DIAGNOSTICS:Before detaching from MPLABCommTool plugnplay
209 1697710031325 GEN4_CONNECT_DIAGNOSTICS:Attaching to MPLABCommTool plugnplay
209 1697710031325 GEN4_CONNECT_DIAGNOSTICS:Calling Update on plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@1cc5184c
209 1697710031325 GEN4_CONNECT_DIAGNOSTICS:Entering plug and play Update(). Attached PID = 9012
209 1697710031325 GEN4_CONNECT_DIAGNOSTICS:Entering MPLABCommEvent handler
209 1697710031325 GEN4_CONNECT_DIAGNOSTICS:MPLABCommEvent.pid = 9012
209 1697710031325 GEN4_CONNECT_DIAGNOSTICS:eventType = MPLABCOMM_TOOL_PLUGGEDIN

209 1697710031325 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
209 1697710031325 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
209 1697710031325 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
209 1697710031325 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.00.85, fpgaVer = ff.ff.ff, scriptVer = 00.05.85, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = d33d758f73, PCB_ID = 4
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
209 1697710031333 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
209 1697710031333 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
209 1697710031333 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
209 1697710031333 GEN4_CONNECT_DIAGNOSTICS:uMode = checkingVersions
209 1697710031333 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
209 1697710031333 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
209 1697710031333 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
209 1697710031333 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4

209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@47674227
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
209 1697710031333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
209 1697710031340 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
209 1697710031340 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
209 1697710031340 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
209 1697710031340 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.00.85, fpgaVer = ff.ff.ff, scriptVer = 00.05.85, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = d33d758f73, PCB_ID = 4
209 1697710031340 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
209 1697710031345 GEN4_CONNECT_DIAGNOSTICS:appNeedsUpdate returned false
209 1697710031345 GEN4_CONNECT_DIAGNOSTICS:Exiting plug and play Update()

659 1697710035965 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
659 1697710035965 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
659 1697710035965 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@47674227
659 1697710035965 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
659 1697710035965 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
659 1697710035965 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
659 1697710035965 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
659 1697710035965 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

659 1697710035965 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
659 1697710035965 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
659 1697710035965 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
659 1697710035965 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
659 1697710035972 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
659 1697710035972 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
659 1697710035972 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
659 1697710035972 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.00.85, fpgaVer = ff.ff.ff, scriptVer = 00.05.85, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = d33d758f73, PCB_ID = 4
659 1697710035972 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
659 1697710035972 XXXX 1697710035972, Thread 659: XXXX 1697710035972, Entering Thread 659: Commands::runScriptWithUpload with script contents. contents[0] = 0x5e, ...  
659 1697710035972 XXXX 1697710035972, Thread 659: XXXX 1697710035972, Entering Thread 659: ToolCommUsb::readTransfer, sideData is 0xd bytes long, transferDataLength is 0x4 bytes long  
659 1697710035973 XXXX 1697710035973, Thread 659: XXXX 1697710035973, Exiting Thread 659: ToolCommUsb::readTransfer,  cr.status = 0x0  
659 1697710035973 XXXX 1697710035973, Thread 659: XXXX 1697710035973, Exiting Thread 659: Commands::runScriptWithUpload  

659 1697710035974 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetPowerInfo
659 1697710035974 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
659 1697710035974 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: Values:
659 1697710035974 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: shotDownSystem = false, isToolPower = true, voltage = 3.250000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
659 1697710035974 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
659 1697710035974 XXXX 1697710035974, Thread 659: XXXX 1697710035974, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
659 1697710035975 XXXX 1697710035975, Thread 659: XXXX 1697710035975, Exiting Thread 659: Commands::runScriptBasic  
659 1697710035975 XXXX 1697710035975, Thread 659: XXXX 1697710035975, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
659 1697710035976 XXXX 1697710035976, Thread 659: XXXX 1697710035976, Exiting Thread 659: Commands::runScriptBasic  
659 1697710035976 XXXX 1697710035976, Thread 659: XXXX 1697710035976, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
659 1697710035988 XXXX 1697710035988, Thread 659: XXXX 1697710035988, Exiting Thread 659: Commands::runScriptBasic  
659 1697710035988 XXXX 1697710035988, Thread 659: XXXX 1697710035988, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
659 1697710036165 XXXX 1697710036165, Thread 659: XXXX 1697710036165, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036165 XXXX 1697710036165, Thread 659: XXXX 1697710036165, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
659 1697710036170 XXXX 1697710036170, Thread 659: XXXX 1697710036170, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036170 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetPowerInfo
659 1697710036170 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
659 1697710036170 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
659 1697710036170 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

659 1697710036170 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetLEDBrightness
659 1697710036170 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
659 1697710036170 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H 5
659 1697710036170 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
659 1697710036170 XXXX 1697710036170, Thread 659: XXXX 1697710036170, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0xcf, ...  
659 1697710036171 XXXX 1697710036171, Thread 659: XXXX 1697710036171, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetLEDBrightness
659 1697710036171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
659 1697710036171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
659 1697710036171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

659 1697710036171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetToolInfo
659 1697710036171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
659 1697710036171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: Values:
659 1697710036171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: speedLevel = 1, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
659 1697710036171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
659 1697710036171 XXXX 1697710036171, Thread 659: XXXX 1697710036171, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
659 1697710036172 XXXX 1697710036172, Thread 659: XXXX 1697710036171, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036172 XXXX 1697710036172, Thread 659: XXXX 1697710036172, Entering Thread 659: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
659 1697710036173 XXXX 1697710036173, Thread 659: XXXX 1697710036172, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036173 XXXX 1697710036173, Thread 659: XXXX 1697710036173, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
659 1697710036174 XXXX 1697710036174, Thread 659: XXXX 1697710036173, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036174 XXXX 1697710036174, Thread 659: XXXX 1697710036174, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0xec, ...  
659 1697710036174 XXXX 1697710036174, Thread 659: XXXX 1697710036174, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036175 XXXX 1697710036175, Thread 659: XXXX 1697710036175, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
659 1697710036176 XXXX 1697710036176, Thread 659: XXXX 1697710036176, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036176 XXXX 1697710036176, Thread 659: XXXX 1697710036176, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
659 1697710036177 XXXX 1697710036177, Thread 659: XXXX 1697710036177, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036177 XXXX 1697710036177, Thread 659: XXXX 1697710036177, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
659 1697710036178 XXXX 1697710036178, Thread 659: XXXX 1697710036178, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036178 XXXX 1697710036178, Thread 659: XXXX 1697710036178, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
659 1697710036179 XXXX 1697710036179, Thread 659: XXXX 1697710036179, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036179 XXXX 1697710036179, Thread 659: XXXX 1697710036179, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
659 1697710036180 XXXX 1697710036180, Thread 659: XXXX 1697710036180, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036180 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetToolInfo
659 1697710036180 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
659 1697710036180 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
659 1697710036180 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

659 1697710036186 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
659 1697710036186 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
659 1697710036186 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
659 1697710036186 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = erase, Mask = 00000000, Erase = false, Production Mode = true
659 1697710036186 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 0, Type = Pgm, Mask = 00000000
659 1697710036186 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 0, Type = Cfg, Mask = 00000000
659 1697710036186 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc02fef, Buffer Length = 0, Type = BootFlash, Mask = 00000000
659 1697710036186 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
659 1697710036186 XXXX 1697710036186, Thread 659: XXXX 1697710036186, Entering Thread 659: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
659 1697710036192 XXXX 1697710036192, Thread 659: XXXX 1697710036192, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036192 XXXX 1697710036192, Thread 659: XXXX 1697710036192, Entering Thread 659: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
659 1697710036193 XXXX 1697710036193, Thread 659: XXXX 1697710036193, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036193 XXXX 1697710036193, Thread 659: XXXX 1697710036193, Entering Thread 659: Commands::runScriptBasic, script name = EraseChip, timeOut = 30000 ms  
659 1697710036295 XXXX 1697710036295, Thread 659: XXXX 1697710036295, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036295 XXXX 1697710036295, Thread 659: XXXX 1697710036295, Entering Thread 659: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
659 1697710036296 XXXX 1697710036296, Thread 659: XXXX 1697710036296, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036297 XXXX 1697710036297, Thread 659: XXXX 1697710036297, Entering Thread 659: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
659 1697710036303 XXXX 1697710036303, Thread 659: XXXX 1697710036303, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036303 XXXX 1697710036303, Thread 659: XXXX 1697710036303, Entering Thread 659: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
659 1697710036304 XXXX 1697710036304, Thread 659: XXXX 1697710036304, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036304 XXXX 1697710036304, Thread 659: XXXX 1697710036304, Entering Thread 659: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
659 1697710036305 XXXX 1697710036305, Thread 659: XXXX 1697710036305, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036305 XXXX 1697710036305, Thread 659: XXXX 1697710036305, Entering Thread 659: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
659 1697710036306 XXXX 1697710036306, Thread 659: XXXX 1697710036306, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036306 XXXX 1697710036306, Thread 659: XXXX 1697710036306, Entering Thread 659: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
659 1697710036307 XXXX 1697710036307, Thread 659: XXXX 1697710036307, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036307 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
659 1697710036307 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
659 1697710036307 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
659 1697710036307 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

659 1697710036309 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
659 1697710036309 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
659 1697710036309 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
659 1697710036309 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = write, Mask = 00000000, Erase = false, Production Mode = true
659 1697710036310 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 524288, Type = Pgm, Mask = 00000000
659 1697710036310 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 16, Type = Cfg, Mask = 00000000
659 1697710036310 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc01fff, Buffer Length = 8192, Type = BootFlash, Mask = 00000000
659 1697710036310 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
659 1697710036310 XXXX 1697710036310, Thread 659: XXXX 1697710036310, Entering Thread 659: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
659 1697710036311 XXXX 1697710036311, Thread 659: XXXX 1697710036311, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036311 XXXX 1697710036311, Thread 659: XXXX 1697710036311, Entering Thread 659: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
659 1697710036312 XXXX 1697710036312, Thread 659: XXXX 1697710036312, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036312 XXXX 1697710036312, Thread 659: XXXX 1697710036312, Entering Thread 659: Commands::runScriptBasic, script name = SetupSerialMode, timeOut = -1 ms  
659 1697710036313 XXXX 1697710036313, Thread 659: XXXX 1697710036313, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036313 XXXX 1697710036313, Thread 659: XXXX 1697710036313, Entering Thread 659: Commands::runScriptBasic, script name = LoadLoader, timeOut = -1 ms  
659 1697710036338 XXXX 1697710036338, Thread 659: XXXX 1697710036338, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036338 XXXX 1697710036338, Thread 659: XXXX 1697710036338, Entering Thread 659: Commands::runScriptWithDownload, script name = DownloadPE  
659 1697710036409 XXXX 1697710036409, Thread 659: XXXX 1697710036409, Exiting Thread 659: Commands::runScriptWithDownload(DownloadPE)  
659 1697710036409 XXXX 1697710036409, Thread 659: XXXX 1697710036409, Entering Thread 659: Commands::runScriptBasic, script name = TestPEConnect, timeOut = -1 ms  
659 1697710036410 XXXX 1697710036410, Thread 659: XXXX 1697710036410, Exiting Thread 659: Commands::runScriptBasic  
659 1697710036410 XXXX 1697710036410, Thread 659: XXXX 1697710036410, Entering Thread 659: Commands::runScriptWithDownload, script name = WriteProgmemPE  
659 1697710045153 XXXX 1697710045153, Thread 659: XXXX 1697710045153, Exiting Thread 659: Commands::runScriptWithDownload(WriteProgmemPE)  
659 1697710045153 XXXX 1697710045153, Thread 659: XXXX 1697710045153, Entering Thread 659: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
659 1697710045217 XXXX 1697710045217, Thread 659: XXXX 1697710045217, Exiting Thread 659: Commands::runScriptBasic  
659 1697710045217 XXXX 1697710045217, Thread 659: XXXX 1697710045217, Entering Thread 659: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
659 1697710045281 XXXX 1697710045281, Thread 659: XXXX 1697710045281, Exiting Thread 659: Commands::runScriptBasic  
659 1697710045281 XXXX 1697710045281, Thread 659: XXXX 1697710045281, Entering Thread 659: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
659 1697710045345 XXXX 1697710045345, Thread 659: XXXX 1697710045345, Exiting Thread 659: Commands::runScriptBasic  
659 1697710045345 XXXX 1697710045345, Thread 659: XXXX 1697710045345, Entering Thread 659: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
659 1697710045409 XXXX 1697710045409, Thread 659: XXXX 1697710045409, Exiting Thread 659: Commands::runScriptBasic  
659 1697710045409 XXXX 1697710045409, Thread 659: XXXX 1697710045409, Entering Thread 659: Commands::runScriptWithDownload, script name = WriteConfigmemPE  
659 1697710045412 XXXX 1697710045412, Thread 659: XXXX 1697710045412, Exiting Thread 659: Commands::runScriptWithDownload(WriteConfigmemPE)  
659 1697710045412 XXXX 1697710045412, Thread 659: XXXX 1697710045412, Entering Thread 659: Commands::runScriptWithUpload, script name = ReadProgmemPE  
659 1697710045412 XXXX 1697710045412, Thread 659: XXXX 1697710045412, Entering Thread 659: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x10 bytes long  
659 1697710045414 XXXX 1697710045414, Thread 659: XXXX 1697710045414, Exiting Thread 659: ToolCommUsb::readTransfer,  cr.status = 0x0  
659 1697710045414 XXXX 1697710045414, Thread 659: XXXX 1697710045414, Exiting Thread 659: Commands::runScriptWithUpload  
659 1697710045414 XXXX 1697710045414, Thread 659: XXXX 1697710045414, Entering Thread 659: Commands::runScriptWithDownload, script name = WriteProgmemPE  
659 1697710045555 XXXX 1697710045555, Thread 659: XXXX 1697710045555, Exiting Thread 659: Commands::runScriptWithDownload(WriteProgmemPE)  
659 1697710045555 XXXX 1697710045555, Thread 659: XXXX 1697710045555, Entering Thread 659: Commands::runScriptWithUpload, script name = ReadProgmemPE  
659 1697710045556 XXXX 1697710045556, Thread 659: XXXX 1697710045556, Entering Thread 659: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x2000 bytes long  
659 1697710045691 XXXX 1697710045691, Thread 659: XXXX 1697710045691, Exiting Thread 659: ToolCommUsb::readTransfer,  cr.status = 0x0  
659 1697710045691 XXXX 1697710045691, Thread 659: XXXX 1697710045691, Exiting Thread 659: Commands::runScriptWithUpload  
659 1697710045691 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
659 1697710045691 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
659 1697710045691 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
659 1697710045691 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

659 1697710045691 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:endOfOperations
659 1697710045691 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
659 1697710045691 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H null
659 1697710045691 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
659 1697710045691 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:endOfOperations
659 1697710045691 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
659 1697710045691 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
659 1697710045691 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

659 1697710045693 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
659 1697710045693 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
659 1697710045693 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
659 1697710045693 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = releasefromreset, Mask = 00000000, Erase = false, Production Mode = true
659 1697710045693 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
659 1697710045693 XXXX 1697710045693, Thread 659: XXXX 1697710045693, Entering Thread 659: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
659 1697710045695 XXXX 1697710045695, Thread 659: XXXX 1697710045695, Exiting Thread 659: Commands::runScriptBasic  
659 1697710045695 XXXX 1697710045695, Thread 659: XXXX 1697710045695, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0x42, ...  
659 1697710045696 XXXX 1697710045696, Thread 659: XXXX 1697710045696, Exiting Thread 659: Commands::runScriptBasic  
659 1697710045696 XXXX 1697710045696, Thread 659: XXXX 1697710045696, Entering Thread 659: Commands::runScriptBasic with script contents. contents[0] = 0xef, ...  
659 1697710045707 XXXX 1697710045707, Thread 659: XXXX 1697710045707, Exiting Thread 659: Commands::runScriptBasic  
659 1697710045707 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
659 1697710045707 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
659 1697710045707 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
659 1697710045707 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End
209 1697710051743 GEN4_CONNECT_DIAGNOSTICS:Calling Update on plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@1cc5184c
209 1697710051743 GEN4_CONNECT_DIAGNOSTICS:Entering plug and play Update(). Attached PID = 9012
209 1697710051743 GEN4_CONNECT_DIAGNOSTICS:Entering MPLABCommEvent handler
209 1697710051743 GEN4_CONNECT_DIAGNOSTICS:MPLABCommEvent.pid = 9012
209 1697710051743 GEN4_CONNECT_DIAGNOSTICS:eventType = MPLABCOMM_TOOL_UNPLUGGED
209 1697710051743 GEN4_CONNECT_DIAGNOSTICS:Exiting plug and play Update()
209 1697710156326 GEN4_CONNECT_DIAGNOSTICS:Before MPLABCommTool.Connect()
209 1697710156326 GEN4_CONNECT_DIAGNOSTICS:After MPLABCommTool.Connect()
209 1697710156326 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool.Connect() returned MPLABCOMM_NO_ERROR
209 1697710156326 GEN4_CONNECT_DIAGNOSTICS:Before detaching from MPLABCommTool plugnplay
209 1697710156326 GEN4_CONNECT_DIAGNOSTICS:Attaching to MPLABCommTool plugnplay
209 1697710156326 GEN4_CONNECT_DIAGNOSTICS:Calling Update on plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@1cc5184c
209 1697710156326 GEN4_CONNECT_DIAGNOSTICS:Entering plug and play Update(). Attached PID = 9012
209 1697710156326 GEN4_CONNECT_DIAGNOSTICS:Entering MPLABCommEvent handler
209 1697710156326 GEN4_CONNECT_DIAGNOSTICS:MPLABCommEvent.pid = 9012
209 1697710156326 GEN4_CONNECT_DIAGNOSTICS:eventType = MPLABCOMM_TOOL_PLUGGEDIN

209 1697710156326 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
209 1697710156326 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
209 1697710156326 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
209 1697710156326 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
209 1697710156333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
209 1697710156333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
209 1697710156333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
209 1697710156333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.00.85, fpgaVer = ff.ff.ff, scriptVer = 00.05.85, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = d33d758f73, PCB_ID = 4
209 1697710156333 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
209 1697710156333 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
209 1697710156333 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
209 1697710156333 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
209 1697710156333 GEN4_CONNECT_DIAGNOSTICS:uMode = done
209 1697710156333 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
209 1697710156333 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
209 1697710156333 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
209 1697710156333 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.updatePk4HybridFirmware()
209 1697710156333 GEN4_CONNECT_DIAGNOSTICS:Don't upgrade fimware = false
209 1697710156333 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.updatePk4HybridFirmware()
209 1697710156333 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
209 1697710156333 GEN4_CONNECT_DIAGNOSTICS:Exiting plug and play Update()

682 1697710161598 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
682 1697710161598 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
682 1697710161598 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@47674227
682 1697710161598 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
682 1697710161598 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
682 1697710161598 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
682 1697710161598 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
682 1697710161598 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

682 1697710161598 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
682 1697710161598 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
682 1697710161598 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
682 1697710161598 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
682 1697710161605 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
682 1697710161605 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
682 1697710161605 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
682 1697710161605 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.00.85, fpgaVer = ff.ff.ff, scriptVer = 00.05.85, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = d33d758f73, PCB_ID = 4
682 1697710161605 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
682 1697710161605 XXXX 1697710161605, Thread 682: XXXX 1697710161605, Entering Thread 682: Commands::runScriptWithUpload with script contents. contents[0] = 0x5e, ...  
682 1697710161605 XXXX 1697710161605, Thread 682: XXXX 1697710161605, Entering Thread 682: ToolCommUsb::readTransfer, sideData is 0xd bytes long, transferDataLength is 0x4 bytes long  
682 1697710161606 XXXX 1697710161606, Thread 682: XXXX 1697710161606, Exiting Thread 682: ToolCommUsb::readTransfer,  cr.status = 0x0  
682 1697710161606 XXXX 1697710161606, Thread 682: XXXX 1697710161606, Exiting Thread 682: Commands::runScriptWithUpload  

682 1697710161606 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetPowerInfo
682 1697710161606 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
682 1697710161606 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: Values:
682 1697710161606 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: shotDownSystem = false, isToolPower = true, voltage = 3.250000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
682 1697710161606 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
682 1697710161606 XXXX 1697710161606, Thread 682: XXXX 1697710161606, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
682 1697710161607 XXXX 1697710161607, Thread 682: XXXX 1697710161607, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161607 XXXX 1697710161607, Thread 682: XXXX 1697710161607, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
682 1697710161608 XXXX 1697710161608, Thread 682: XXXX 1697710161608, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161608 XXXX 1697710161608, Thread 682: XXXX 1697710161608, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
682 1697710161621 XXXX 1697710161621, Thread 682: XXXX 1697710161621, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161621 XXXX 1697710161621, Thread 682: XXXX 1697710161621, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
682 1697710161798 XXXX 1697710161798, Thread 682: XXXX 1697710161798, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161798 XXXX 1697710161798, Thread 682: XXXX 1697710161798, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
682 1697710161803 XXXX 1697710161803, Thread 682: XXXX 1697710161803, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161803 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetPowerInfo
682 1697710161803 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
682 1697710161803 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
682 1697710161803 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

682 1697710161803 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetLEDBrightness
682 1697710161803 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
682 1697710161803 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H 5
682 1697710161803 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
682 1697710161803 XXXX 1697710161803, Thread 682: XXXX 1697710161803, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0xcf, ...  
682 1697710161804 XXXX 1697710161804, Thread 682: XXXX 1697710161804, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161804 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetLEDBrightness
682 1697710161804 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
682 1697710161804 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
682 1697710161804 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

682 1697710161804 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetToolInfo
682 1697710161804 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
682 1697710161804 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: Values:
682 1697710161804 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: speedLevel = 1, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
682 1697710161804 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
682 1697710161804 XXXX 1697710161804, Thread 682: XXXX 1697710161804, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
682 1697710161805 XXXX 1697710161805, Thread 682: XXXX 1697710161805, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161805 XXXX 1697710161805, Thread 682: XXXX 1697710161805, Entering Thread 682: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
682 1697710161806 XXXX 1697710161806, Thread 682: XXXX 1697710161806, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161806 XXXX 1697710161806, Thread 682: XXXX 1697710161806, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
682 1697710161807 XXXX 1697710161807, Thread 682: XXXX 1697710161807, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161807 XXXX 1697710161807, Thread 682: XXXX 1697710161807, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0xec, ...  
682 1697710161808 XXXX 1697710161808, Thread 682: XXXX 1697710161808, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161808 XXXX 1697710161808, Thread 682: XXXX 1697710161808, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
682 1697710161809 XXXX 1697710161809, Thread 682: XXXX 1697710161809, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161809 XXXX 1697710161809, Thread 682: XXXX 1697710161809, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
682 1697710161810 XXXX 1697710161810, Thread 682: XXXX 1697710161810, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161810 XXXX 1697710161810, Thread 682: XXXX 1697710161810, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
682 1697710161811 XXXX 1697710161811, Thread 682: XXXX 1697710161811, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161811 XXXX 1697710161811, Thread 682: XXXX 1697710161811, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
682 1697710161812 XXXX 1697710161812, Thread 682: XXXX 1697710161812, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161812 XXXX 1697710161812, Thread 682: XXXX 1697710161812, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
682 1697710161813 XXXX 1697710161813, Thread 682: XXXX 1697710161813, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161813 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetToolInfo
682 1697710161813 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
682 1697710161813 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
682 1697710161813 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

682 1697710161819 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
682 1697710161819 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
682 1697710161819 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
682 1697710161819 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = erase, Mask = 00000000, Erase = false, Production Mode = true
682 1697710161819 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 0, Type = Pgm, Mask = 00000000
682 1697710161819 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 0, Type = Cfg, Mask = 00000000
682 1697710161819 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc02fef, Buffer Length = 0, Type = BootFlash, Mask = 00000000
682 1697710161819 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
682 1697710161819 XXXX 1697710161819, Thread 682: XXXX 1697710161819, Entering Thread 682: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
682 1697710161825 XXXX 1697710161825, Thread 682: XXXX 1697710161825, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161825 XXXX 1697710161825, Thread 682: XXXX 1697710161825, Entering Thread 682: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
682 1697710161826 XXXX 1697710161826, Thread 682: XXXX 1697710161826, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161826 XXXX 1697710161826, Thread 682: XXXX 1697710161826, Entering Thread 682: Commands::runScriptBasic, script name = EraseChip, timeOut = 30000 ms  
682 1697710161928 XXXX 1697710161928, Thread 682: XXXX 1697710161928, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161928 XXXX 1697710161928, Thread 682: XXXX 1697710161928, Entering Thread 682: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
682 1697710161930 XXXX 1697710161930, Thread 682: XXXX 1697710161930, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161930 XXXX 1697710161930, Thread 682: XXXX 1697710161930, Entering Thread 682: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
682 1697710161936 XXXX 1697710161936, Thread 682: XXXX 1697710161936, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161936 XXXX 1697710161936, Thread 682: XXXX 1697710161936, Entering Thread 682: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
682 1697710161937 XXXX 1697710161937, Thread 682: XXXX 1697710161937, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161937 XXXX 1697710161937, Thread 682: XXXX 1697710161937, Entering Thread 682: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
682 1697710161938 XXXX 1697710161938, Thread 682: XXXX 1697710161938, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161938 XXXX 1697710161938, Thread 682: XXXX 1697710161938, Entering Thread 682: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
682 1697710161939 XXXX 1697710161939, Thread 682: XXXX 1697710161939, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161939 XXXX 1697710161939, Thread 682: XXXX 1697710161939, Entering Thread 682: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
682 1697710161940 XXXX 1697710161940, Thread 682: XXXX 1697710161940, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161940 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
682 1697710161940 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
682 1697710161940 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
682 1697710161940 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

682 1697710161942 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
682 1697710161942 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
682 1697710161942 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
682 1697710161942 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = write, Mask = 00000000, Erase = false, Production Mode = true
682 1697710161942 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 524288, Type = Pgm, Mask = 00000000
682 1697710161942 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 16, Type = Cfg, Mask = 00000000
682 1697710161942 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc01fff, Buffer Length = 8192, Type = BootFlash, Mask = 00000000
682 1697710161942 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
682 1697710161943 XXXX 1697710161943, Thread 682: XXXX 1697710161943, Entering Thread 682: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
682 1697710161944 XXXX 1697710161944, Thread 682: XXXX 1697710161944, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161944 XXXX 1697710161944, Thread 682: XXXX 1697710161944, Entering Thread 682: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
682 1697710161945 XXXX 1697710161945, Thread 682: XXXX 1697710161945, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161945 XXXX 1697710161945, Thread 682: XXXX 1697710161945, Entering Thread 682: Commands::runScriptBasic, script name = SetupSerialMode, timeOut = -1 ms  
682 1697710161946 XXXX 1697710161946, Thread 682: XXXX 1697710161946, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161946 XXXX 1697710161946, Thread 682: XXXX 1697710161946, Entering Thread 682: Commands::runScriptBasic, script name = LoadLoader, timeOut = -1 ms  
682 1697710161971 XXXX 1697710161971, Thread 682: XXXX 1697710161971, Exiting Thread 682: Commands::runScriptBasic  
682 1697710161971 XXXX 1697710161971, Thread 682: XXXX 1697710161971, Entering Thread 682: Commands::runScriptWithDownload, script name = DownloadPE  
682 1697710162042 XXXX 1697710162042, Thread 682: XXXX 1697710162042, Exiting Thread 682: Commands::runScriptWithDownload(DownloadPE)  
682 1697710162042 XXXX 1697710162042, Thread 682: XXXX 1697710162042, Entering Thread 682: Commands::runScriptBasic, script name = TestPEConnect, timeOut = -1 ms  
682 1697710162043 XXXX 1697710162043, Thread 682: XXXX 1697710162043, Exiting Thread 682: Commands::runScriptBasic  
682 1697710162043 XXXX 1697710162043, Thread 682: XXXX 1697710162043, Entering Thread 682: Commands::runScriptWithDownload, script name = WriteProgmemPE  
682 1697710170785 XXXX 1697710170785, Thread 682: XXXX 1697710170785, Exiting Thread 682: Commands::runScriptWithDownload(WriteProgmemPE)  
682 1697710170785 XXXX 1697710170785, Thread 682: XXXX 1697710170785, Entering Thread 682: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
682 1697710170848 XXXX 1697710170848, Thread 682: XXXX 1697710170848, Exiting Thread 682: Commands::runScriptBasic  
682 1697710170849 XXXX 1697710170849, Thread 682: XXXX 1697710170849, Entering Thread 682: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
682 1697710170912 XXXX 1697710170912, Thread 682: XXXX 1697710170912, Exiting Thread 682: Commands::runScriptBasic  
682 1697710170913 XXXX 1697710170913, Thread 682: XXXX 1697710170913, Entering Thread 682: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
682 1697710170976 XXXX 1697710170976, Thread 682: XXXX 1697710170976, Exiting Thread 682: Commands::runScriptBasic  
682 1697710170977 XXXX 1697710170977, Thread 682: XXXX 1697710170977, Entering Thread 682: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
682 1697710171040 XXXX 1697710171040, Thread 682: XXXX 1697710171040, Exiting Thread 682: Commands::runScriptBasic  
682 1697710171041 XXXX 1697710171041, Thread 682: XXXX 1697710171041, Entering Thread 682: Commands::runScriptWithDownload, script name = WriteConfigmemPE  
682 1697710171043 XXXX 1697710171043, Thread 682: XXXX 1697710171043, Exiting Thread 682: Commands::runScriptWithDownload(WriteConfigmemPE)  
682 1697710171043 XXXX 1697710171043, Thread 682: XXXX 1697710171043, Entering Thread 682: Commands::runScriptWithUpload, script name = ReadProgmemPE  
682 1697710171043 XXXX 1697710171043, Thread 682: XXXX 1697710171043, Entering Thread 682: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x10 bytes long  
682 1697710171045 XXXX 1697710171045, Thread 682: XXXX 1697710171045, Exiting Thread 682: ToolCommUsb::readTransfer,  cr.status = 0x0  
682 1697710171045 XXXX 1697710171045, Thread 682: XXXX 1697710171045, Exiting Thread 682: Commands::runScriptWithUpload  
682 1697710171045 XXXX 1697710171045, Thread 682: XXXX 1697710171045, Entering Thread 682: Commands::runScriptWithDownload, script name = WriteProgmemPE  
682 1697710171188 XXXX 1697710171188, Thread 682: XXXX 1697710171188, Exiting Thread 682: Commands::runScriptWithDownload(WriteProgmemPE)  
682 1697710171188 XXXX 1697710171188, Thread 682: XXXX 1697710171188, Entering Thread 682: Commands::runScriptWithUpload, script name = ReadProgmemPE  
682 1697710171188 XXXX 1697710171188, Thread 682: XXXX 1697710171188, Entering Thread 682: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x2000 bytes long  
682 1697710171324 XXXX 1697710171324, Thread 682: XXXX 1697710171324, Exiting Thread 682: ToolCommUsb::readTransfer,  cr.status = 0x0  
682 1697710171324 XXXX 1697710171324, Thread 682: XXXX 1697710171324, Exiting Thread 682: Commands::runScriptWithUpload  
682 1697710171324 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
682 1697710171324 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
682 1697710171324 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
682 1697710171324 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

682 1697710171324 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:endOfOperations
682 1697710171324 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
682 1697710171324 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H null
682 1697710171324 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
682 1697710171324 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:endOfOperations
682 1697710171324 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
682 1697710171324 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
682 1697710171324 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

682 1697710171326 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
682 1697710171326 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
682 1697710171326 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
682 1697710171326 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = releasefromreset, Mask = 00000000, Erase = false, Production Mode = true
682 1697710171326 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
682 1697710171326 XXXX 1697710171326, Thread 682: XXXX 1697710171326, Entering Thread 682: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
682 1697710171328 XXXX 1697710171328, Thread 682: XXXX 1697710171328, Exiting Thread 682: Commands::runScriptBasic  
682 1697710171328 XXXX 1697710171328, Thread 682: XXXX 1697710171328, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0x42, ...  
682 1697710171329 XXXX 1697710171329, Thread 682: XXXX 1697710171329, Exiting Thread 682: Commands::runScriptBasic  
682 1697710171329 XXXX 1697710171329, Thread 682: XXXX 1697710171329, Entering Thread 682: Commands::runScriptBasic with script contents. contents[0] = 0xef, ...  
682 1697710171340 XXXX 1697710171340, Thread 682: XXXX 1697710171340, Exiting Thread 682: Commands::runScriptBasic  
682 1697710171340 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
682 1697710171340 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
682 1697710171340 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
682 1697710171340 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End
209 1697710175742 GEN4_CONNECT_DIAGNOSTICS:Calling Update on plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@1cc5184c
209 1697710175742 GEN4_CONNECT_DIAGNOSTICS:Entering plug and play Update(). Attached PID = 9012
209 1697710175742 GEN4_CONNECT_DIAGNOSTICS:Entering MPLABCommEvent handler
209 1697710175742 GEN4_CONNECT_DIAGNOSTICS:MPLABCommEvent.pid = 9012
209 1697710175742 GEN4_CONNECT_DIAGNOSTICS:eventType = MPLABCOMM_TOOL_UNPLUGGED
209 1697710175742 GEN4_CONNECT_DIAGNOSTICS:Exiting plug and play Update()
209 1697713868327 GEN4_CONNECT_DIAGNOSTICS:Before MPLABCommTool.Connect()
209 1697713868327 GEN4_CONNECT_DIAGNOSTICS:After MPLABCommTool.Connect()
209 1697713868327 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool.Connect() returned MPLABCOMM_NO_ERROR
209 1697713868327 GEN4_CONNECT_DIAGNOSTICS:Before detaching from MPLABCommTool plugnplay
209 1697713868327 GEN4_CONNECT_DIAGNOSTICS:Attaching to MPLABCommTool plugnplay
209 1697713868327 GEN4_CONNECT_DIAGNOSTICS:Calling Update on plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@1cc5184c
209 1697713868327 GEN4_CONNECT_DIAGNOSTICS:Entering plug and play Update(). Attached PID = 9012
209 1697713868327 GEN4_CONNECT_DIAGNOSTICS:Entering MPLABCommEvent handler
209 1697713868327 GEN4_CONNECT_DIAGNOSTICS:MPLABCommEvent.pid = 9012
209 1697713868327 GEN4_CONNECT_DIAGNOSTICS:eventType = MPLABCOMM_TOOL_PLUGGEDIN

209 1697713868327 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
209 1697713868327 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
209 1697713868327 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
209 1697713868327 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.00.85, fpgaVer = ff.ff.ff, scriptVer = 00.05.85, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = d33d758f73, PCB_ID = 4
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
209 1697713868334 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
209 1697713868334 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
209 1697713868334 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
209 1697713868334 GEN4_CONNECT_DIAGNOSTICS:uMode = checkingVersions
209 1697713868334 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
209 1697713868334 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
209 1697713868334 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
209 1697713868334 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4

209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@47674227
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
209 1697713868334 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
209 1697713868342 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
209 1697713868342 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
209 1697713868342 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
209 1697713868342 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.00.85, fpgaVer = ff.ff.ff, scriptVer = 00.05.85, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = d33d758f73, PCB_ID = 4
209 1697713868342 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
209 1697713868357 GEN4_CONNECT_DIAGNOSTICS:appNeedsUpdate returned false
209 1697713868357 GEN4_CONNECT_DIAGNOSTICS:Exiting plug and play Update()

735 1697713921983 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
735 1697713921983 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
735 1697713921983 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@47674227
735 1697713921983 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
735 1697713921983 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
735 1697713921983 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
735 1697713921983 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
735 1697713921983 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

735 1697713921983 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
735 1697713921983 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
735 1697713921983 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
735 1697713921983 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
735 1697713921991 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
735 1697713921991 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
735 1697713921991 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
735 1697713921991 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.00.85, fpgaVer = ff.ff.ff, scriptVer = 00.05.85, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = d33d758f73, PCB_ID = 4
735 1697713921991 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
735 1697713921991 XXXX 1697713921991, Thread 735: XXXX 1697713921991, Entering Thread 735: Commands::runScriptWithUpload with script contents. contents[0] = 0x5e, ...  
735 1697713921991 XXXX 1697713921991, Thread 735: XXXX 1697713921991, Entering Thread 735: ToolCommUsb::readTransfer, sideData is 0xd bytes long, transferDataLength is 0x4 bytes long  
735 1697713921992 XXXX 1697713921992, Thread 735: XXXX 1697713921992, Exiting Thread 735: ToolCommUsb::readTransfer,  cr.status = 0x0  
735 1697713921992 XXXX 1697713921992, Thread 735: XXXX 1697713921992, Exiting Thread 735: Commands::runScriptWithUpload  

735 1697713921992 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetPowerInfo
735 1697713921992 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
735 1697713921992 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: Values:
735 1697713921992 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: shotDownSystem = false, isToolPower = true, voltage = 3.250000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
735 1697713921992 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
735 1697713921992 XXXX 1697713921992, Thread 735: XXXX 1697713921992, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
735 1697713921993 XXXX 1697713921993, Thread 735: XXXX 1697713921993, Exiting Thread 735: Commands::runScriptBasic  
735 1697713921993 XXXX 1697713921993, Thread 735: XXXX 1697713921993, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
735 1697713921994 XXXX 1697713921994, Thread 735: XXXX 1697713921994, Exiting Thread 735: Commands::runScriptBasic  
735 1697713921994 XXXX 1697713921994, Thread 735: XXXX 1697713921994, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
735 1697713922007 XXXX 1697713922007, Thread 735: XXXX 1697713922007, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922007 XXXX 1697713922007, Thread 735: XXXX 1697713922007, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
735 1697713922184 XXXX 1697713922184, Thread 735: XXXX 1697713922184, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922184 XXXX 1697713922184, Thread 735: XXXX 1697713922184, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
735 1697713922189 XXXX 1697713922189, Thread 735: XXXX 1697713922189, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922189 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetPowerInfo
735 1697713922189 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
735 1697713922189 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
735 1697713922189 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

735 1697713922189 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetLEDBrightness
735 1697713922189 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
735 1697713922189 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H 5
735 1697713922189 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
735 1697713922189 XXXX 1697713922189, Thread 735: XXXX 1697713922189, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0xcf, ...  
735 1697713922190 XXXX 1697713922190, Thread 735: XXXX 1697713922190, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922190 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetLEDBrightness
735 1697713922190 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
735 1697713922190 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
735 1697713922190 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

735 1697713922190 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetToolInfo
735 1697713922190 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
735 1697713922190 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: Values:
735 1697713922190 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: speedLevel = 1, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
735 1697713922190 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
735 1697713922190 XXXX 1697713922190, Thread 735: XXXX 1697713922190, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
735 1697713922191 XXXX 1697713922191, Thread 735: XXXX 1697713922191, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922191 XXXX 1697713922191, Thread 735: XXXX 1697713922191, Entering Thread 735: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
735 1697713922192 XXXX 1697713922192, Thread 735: XXXX 1697713922192, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922192 XXXX 1697713922192, Thread 735: XXXX 1697713922192, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
735 1697713922193 XXXX 1697713922193, Thread 735: XXXX 1697713922193, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922193 XXXX 1697713922193, Thread 735: XXXX 1697713922193, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0xec, ...  
735 1697713922194 XXXX 1697713922194, Thread 735: XXXX 1697713922194, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922194 XXXX 1697713922194, Thread 735: XXXX 1697713922194, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
735 1697713922195 XXXX 1697713922195, Thread 735: XXXX 1697713922195, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922195 XXXX 1697713922195, Thread 735: XXXX 1697713922195, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
735 1697713922196 XXXX 1697713922196, Thread 735: XXXX 1697713922196, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922196 XXXX 1697713922196, Thread 735: XXXX 1697713922196, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
735 1697713922197 XXXX 1697713922197, Thread 735: XXXX 1697713922197, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922197 XXXX 1697713922197, Thread 735: XXXX 1697713922197, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
735 1697713922198 XXXX 1697713922198, Thread 735: XXXX 1697713922198, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922198 XXXX 1697713922198, Thread 735: XXXX 1697713922198, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
735 1697713922199 XXXX 1697713922199, Thread 735: XXXX 1697713922199, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922199 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetToolInfo
735 1697713922199 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
735 1697713922199 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
735 1697713922199 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

735 1697713922205 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
735 1697713922205 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
735 1697713922205 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
735 1697713922205 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = erase, Mask = 00000000, Erase = false, Production Mode = true
735 1697713922205 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 0, Type = Pgm, Mask = 00000000
735 1697713922205 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 0, Type = Cfg, Mask = 00000000
735 1697713922205 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc02fef, Buffer Length = 0, Type = BootFlash, Mask = 00000000
735 1697713922205 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
735 1697713922205 XXXX 1697713922205, Thread 735: XXXX 1697713922205, Entering Thread 735: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
735 1697713922211 XXXX 1697713922211, Thread 735: XXXX 1697713922211, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922211 XXXX 1697713922211, Thread 735: XXXX 1697713922211, Entering Thread 735: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
735 1697713922212 XXXX 1697713922212, Thread 735: XXXX 1697713922212, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922212 XXXX 1697713922212, Thread 735: XXXX 1697713922212, Entering Thread 735: Commands::runScriptBasic, script name = EraseChip, timeOut = 30000 ms  
735 1697713922313 XXXX 1697713922313, Thread 735: XXXX 1697713922313, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922313 XXXX 1697713922313, Thread 735: XXXX 1697713922313, Entering Thread 735: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
735 1697713922315 XXXX 1697713922315, Thread 735: XXXX 1697713922315, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922315 XXXX 1697713922315, Thread 735: XXXX 1697713922315, Entering Thread 735: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
735 1697713922321 XXXX 1697713922321, Thread 735: XXXX 1697713922321, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922321 XXXX 1697713922321, Thread 735: XXXX 1697713922321, Entering Thread 735: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
735 1697713922322 XXXX 1697713922322, Thread 735: XXXX 1697713922322, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922322 XXXX 1697713922322, Thread 735: XXXX 1697713922322, Entering Thread 735: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
735 1697713922323 XXXX 1697713922323, Thread 735: XXXX 1697713922323, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922323 XXXX 1697713922323, Thread 735: XXXX 1697713922323, Entering Thread 735: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
735 1697713922324 XXXX 1697713922324, Thread 735: XXXX 1697713922324, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922324 XXXX 1697713922324, Thread 735: XXXX 1697713922324, Entering Thread 735: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
735 1697713922325 XXXX 1697713922325, Thread 735: XXXX 1697713922325, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922325 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
735 1697713922325 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
735 1697713922325 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
735 1697713922325 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

735 1697713922328 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
735 1697713922328 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
735 1697713922328 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
735 1697713922328 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = write, Mask = 00000000, Erase = false, Production Mode = true
735 1697713922328 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 524288, Type = Pgm, Mask = 00000000
735 1697713922328 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 16, Type = Cfg, Mask = 00000000
735 1697713922328 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc01fff, Buffer Length = 8192, Type = BootFlash, Mask = 00000000
735 1697713922328 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
735 1697713922328 XXXX 1697713922328, Thread 735: XXXX 1697713922328, Entering Thread 735: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
735 1697713922329 XXXX 1697713922329, Thread 735: XXXX 1697713922329, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922329 XXXX 1697713922329, Thread 735: XXXX 1697713922329, Entering Thread 735: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
735 1697713922330 XXXX 1697713922330, Thread 735: XXXX 1697713922330, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922330 XXXX 1697713922330, Thread 735: XXXX 1697713922330, Entering Thread 735: Commands::runScriptBasic, script name = SetupSerialMode, timeOut = -1 ms  
735 1697713922332 XXXX 1697713922332, Thread 735: XXXX 1697713922332, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922332 XXXX 1697713922332, Thread 735: XXXX 1697713922332, Entering Thread 735: Commands::runScriptBasic, script name = LoadLoader, timeOut = -1 ms  
735 1697713922356 XXXX 1697713922356, Thread 735: XXXX 1697713922356, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922356 XXXX 1697713922356, Thread 735: XXXX 1697713922356, Entering Thread 735: Commands::runScriptWithDownload, script name = DownloadPE  
735 1697713922428 XXXX 1697713922428, Thread 735: XXXX 1697713922428, Exiting Thread 735: Commands::runScriptWithDownload(DownloadPE)  
735 1697713922428 XXXX 1697713922428, Thread 735: XXXX 1697713922428, Entering Thread 735: Commands::runScriptBasic, script name = TestPEConnect, timeOut = -1 ms  
735 1697713922429 XXXX 1697713922429, Thread 735: XXXX 1697713922429, Exiting Thread 735: Commands::runScriptBasic  
735 1697713922429 XXXX 1697713922429, Thread 735: XXXX 1697713922429, Entering Thread 735: Commands::runScriptWithDownload, script name = WriteProgmemPE  
735 1697713931172 XXXX 1697713931172, Thread 735: XXXX 1697713931172, Exiting Thread 735: Commands::runScriptWithDownload(WriteProgmemPE)  
735 1697713931172 XXXX 1697713931172, Thread 735: XXXX 1697713931172, Entering Thread 735: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
735 1697713931235 XXXX 1697713931235, Thread 735: XXXX 1697713931235, Exiting Thread 735: Commands::runScriptBasic  
735 1697713931235 XXXX 1697713931235, Thread 735: XXXX 1697713931235, Entering Thread 735: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
735 1697713931299 XXXX 1697713931299, Thread 735: XXXX 1697713931299, Exiting Thread 735: Commands::runScriptBasic  
735 1697713931300 XXXX 1697713931300, Thread 735: XXXX 1697713931300, Entering Thread 735: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
735 1697713931363 XXXX 1697713931363, Thread 735: XXXX 1697713931363, Exiting Thread 735: Commands::runScriptBasic  
735 1697713931364 XXXX 1697713931364, Thread 735: XXXX 1697713931364, Entering Thread 735: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
735 1697713931428 XXXX 1697713931428, Thread 735: XXXX 1697713931428, Exiting Thread 735: Commands::runScriptBasic  
735 1697713931428 XXXX 1697713931428, Thread 735: XXXX 1697713931428, Entering Thread 735: Commands::runScriptWithDownload, script name = WriteConfigmemPE  
735 1697713931431 XXXX 1697713931431, Thread 735: XXXX 1697713931431, Exiting Thread 735: Commands::runScriptWithDownload(WriteConfigmemPE)  
735 1697713931431 XXXX 1697713931431, Thread 735: XXXX 1697713931431, Entering Thread 735: Commands::runScriptWithUpload, script name = ReadProgmemPE  
735 1697713931431 XXXX 1697713931431, Thread 735: XXXX 1697713931431, Entering Thread 735: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x10 bytes long  
735 1697713931433 XXXX 1697713931433, Thread 735: XXXX 1697713931433, Exiting Thread 735: ToolCommUsb::readTransfer,  cr.status = 0x0  
735 1697713931433 XXXX 1697713931433, Thread 735: XXXX 1697713931433, Exiting Thread 735: Commands::runScriptWithUpload  
735 1697713931433 XXXX 1697713931433, Thread 735: XXXX 1697713931433, Entering Thread 735: Commands::runScriptWithDownload, script name = WriteProgmemPE  
735 1697713931574 XXXX 1697713931574, Thread 735: XXXX 1697713931574, Exiting Thread 735: Commands::runScriptWithDownload(WriteProgmemPE)  
735 1697713931574 XXXX 1697713931574, Thread 735: XXXX 1697713931574, Entering Thread 735: Commands::runScriptWithUpload, script name = ReadProgmemPE  
735 1697713931574 XXXX 1697713931574, Thread 735: XXXX 1697713931574, Entering Thread 735: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x2000 bytes long  
735 1697713931710 XXXX 1697713931710, Thread 735: XXXX 1697713931710, Exiting Thread 735: ToolCommUsb::readTransfer,  cr.status = 0x0  
735 1697713931710 XXXX 1697713931710, Thread 735: XXXX 1697713931710, Exiting Thread 735: Commands::runScriptWithUpload  
735 1697713931710 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
735 1697713931710 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
735 1697713931710 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
735 1697713931710 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

735 1697713931710 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:endOfOperations
735 1697713931710 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
735 1697713931710 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H null
735 1697713931710 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
735 1697713931710 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:endOfOperations
735 1697713931710 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
735 1697713931710 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
735 1697713931710 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

735 1697713931713 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
735 1697713931713 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
735 1697713931713 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
735 1697713931713 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = releasefromreset, Mask = 00000000, Erase = false, Production Mode = true
735 1697713931713 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
735 1697713931713 XXXX 1697713931713, Thread 735: XXXX 1697713931713, Entering Thread 735: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
735 1697713931715 XXXX 1697713931715, Thread 735: XXXX 1697713931715, Exiting Thread 735: Commands::runScriptBasic  
735 1697713931715 XXXX 1697713931715, Thread 735: XXXX 1697713931715, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0x42, ...  
735 1697713931716 XXXX 1697713931716, Thread 735: XXXX 1697713931716, Exiting Thread 735: Commands::runScriptBasic  
735 1697713931716 XXXX 1697713931716, Thread 735: XXXX 1697713931716, Entering Thread 735: Commands::runScriptBasic with script contents. contents[0] = 0xef, ...  
735 1697713931727 XXXX 1697713931727, Thread 735: XXXX 1697713931727, Exiting Thread 735: Commands::runScriptBasic  
735 1697713931727 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
735 1697713931727 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
735 1697713931727 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
735 1697713931727 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End
209 1697713936244 GEN4_CONNECT_DIAGNOSTICS:Calling Update on plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@1cc5184c
209 1697713936244 GEN4_CONNECT_DIAGNOSTICS:Entering plug and play Update(). Attached PID = 9012
209 1697713936244 GEN4_CONNECT_DIAGNOSTICS:Entering MPLABCommEvent handler
209 1697713936244 GEN4_CONNECT_DIAGNOSTICS:MPLABCommEvent.pid = 9012
209 1697713936244 GEN4_CONNECT_DIAGNOSTICS:eventType = MPLABCOMM_TOOL_UNPLUGGED
209 1697713936244 GEN4_CONNECT_DIAGNOSTICS:Exiting plug and play Update()
209 1697714187824 GEN4_CONNECT_DIAGNOSTICS:Before MPLABCommTool.Connect()
209 1697714187824 GEN4_CONNECT_DIAGNOSTICS:After MPLABCommTool.Connect()
209 1697714187824 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool.Connect() returned MPLABCOMM_NO_ERROR
209 1697714187824 GEN4_CONNECT_DIAGNOSTICS:Before detaching from MPLABCommTool plugnplay
209 1697714187824 GEN4_CONNECT_DIAGNOSTICS:Attaching to MPLABCommTool plugnplay
209 1697714187824 GEN4_CONNECT_DIAGNOSTICS:Calling Update on plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@1cc5184c
209 1697714187824 GEN4_CONNECT_DIAGNOSTICS:Entering plug and play Update(). Attached PID = 9012
209 1697714187824 GEN4_CONNECT_DIAGNOSTICS:Entering MPLABCommEvent handler
209 1697714187824 GEN4_CONNECT_DIAGNOSTICS:MPLABCommEvent.pid = 9012
209 1697714187824 GEN4_CONNECT_DIAGNOSTICS:eventType = MPLABCOMM_TOOL_PLUGGEDIN

209 1697714187824 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
209 1697714187824 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
209 1697714187824 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
209 1697714187824 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
209 1697714187831 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
209 1697714187831 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
209 1697714187831 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
209 1697714187831 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.00.85, fpgaVer = ff.ff.ff, scriptVer = 00.05.85, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = d33d758f73, PCB_ID = 4
209 1697714187831 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
209 1697714187831 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
209 1697714187831 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
209 1697714187831 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
209 1697714187831 GEN4_CONNECT_DIAGNOSTICS:uMode = done
209 1697714187831 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
209 1697714187831 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
209 1697714187831 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
209 1697714187831 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.updatePk4HybridFirmware()
209 1697714187831 GEN4_CONNECT_DIAGNOSTICS:Don't upgrade fimware = false
209 1697714187831 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.updatePk4HybridFirmware()
209 1697714187831 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.FirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
209 1697714187831 GEN4_CONNECT_DIAGNOSTICS:Exiting plug and play Update()

755 1697714195920 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
755 1697714195920 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
755 1697714195920 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@47674227
755 1697714195920 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
755 1697714195920 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
755 1697714195920 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
755 1697714195920 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
755 1697714195920 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

755 1697714195920 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
755 1697714195920 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
755 1697714195920 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
755 1697714195920 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
755 1697714195927 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
755 1697714195927 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
755 1697714195927 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
755 1697714195927 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.00.85, fpgaVer = ff.ff.ff, scriptVer = 00.05.85, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = d33d758f73, PCB_ID = 4
755 1697714195927 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
755 1697714195927 XXXX 1697714195927, Thread 755: XXXX 1697714195927, Entering Thread 755: Commands::runScriptWithUpload with script contents. contents[0] = 0x5e, ...  
755 1697714195927 XXXX 1697714195927, Thread 755: XXXX 1697714195927, Entering Thread 755: ToolCommUsb::readTransfer, sideData is 0xd bytes long, transferDataLength is 0x4 bytes long  
755 1697714195929 XXXX 1697714195929, Thread 755: XXXX 1697714195929, Exiting Thread 755: ToolCommUsb::readTransfer,  cr.status = 0x0  
755 1697714195929 XXXX 1697714195929, Thread 755: XXXX 1697714195929, Exiting Thread 755: Commands::runScriptWithUpload  

755 1697714195929 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetPowerInfo
755 1697714195929 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
755 1697714195929 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: Values:
755 1697714195929 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: shotDownSystem = false, isToolPower = true, voltage = 3.250000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
755 1697714195929 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
755 1697714195929 XXXX 1697714195929, Thread 755: XXXX 1697714195929, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
755 1697714195930 XXXX 1697714195930, Thread 755: XXXX 1697714195930, Exiting Thread 755: Commands::runScriptBasic  
755 1697714195930 XXXX 1697714195930, Thread 755: XXXX 1697714195930, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
755 1697714195931 XXXX 1697714195931, Thread 755: XXXX 1697714195931, Exiting Thread 755: Commands::runScriptBasic  
755 1697714195931 XXXX 1697714195931, Thread 755: XXXX 1697714195931, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
755 1697714195943 XXXX 1697714195943, Thread 755: XXXX 1697714195943, Exiting Thread 755: Commands::runScriptBasic  
755 1697714195943 XXXX 1697714195943, Thread 755: XXXX 1697714195943, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
755 1697714196120 XXXX 1697714196120, Thread 755: XXXX 1697714196120, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196120 XXXX 1697714196120, Thread 755: XXXX 1697714196120, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
755 1697714196126 XXXX 1697714196126, Thread 755: XXXX 1697714196126, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196126 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetPowerInfo
755 1697714196126 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
755 1697714196126 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
755 1697714196126 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

755 1697714196126 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetLEDBrightness
755 1697714196126 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
755 1697714196126 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H 5
755 1697714196126 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
755 1697714196126 XXXX 1697714196126, Thread 755: XXXX 1697714196126, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0xcf, ...  
755 1697714196127 XXXX 1697714196127, Thread 755: XXXX 1697714196127, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196127 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetLEDBrightness
755 1697714196127 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
755 1697714196127 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
755 1697714196127 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

755 1697714196127 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetToolInfo
755 1697714196127 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
755 1697714196127 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: Values:
755 1697714196127 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: speedLevel = 1, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
755 1697714196127 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
755 1697714196127 XXXX 1697714196127, Thread 755: XXXX 1697714196127, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
755 1697714196127 XXXX 1697714196127, Thread 755: XXXX 1697714196127, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196127 XXXX 1697714196127, Thread 755: XXXX 1697714196127, Entering Thread 755: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
755 1697714196128 XXXX 1697714196128, Thread 755: XXXX 1697714196128, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196128 XXXX 1697714196128, Thread 755: XXXX 1697714196128, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
755 1697714196129 XXXX 1697714196129, Thread 755: XXXX 1697714196129, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196129 XXXX 1697714196129, Thread 755: XXXX 1697714196129, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0xec, ...  
755 1697714196130 XXXX 1697714196130, Thread 755: XXXX 1697714196130, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196130 XXXX 1697714196130, Thread 755: XXXX 1697714196130, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
755 1697714196131 XXXX 1697714196131, Thread 755: XXXX 1697714196131, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196131 XXXX 1697714196131, Thread 755: XXXX 1697714196131, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
755 1697714196132 XXXX 1697714196132, Thread 755: XXXX 1697714196132, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196132 XXXX 1697714196132, Thread 755: XXXX 1697714196132, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
755 1697714196134 XXXX 1697714196134, Thread 755: XXXX 1697714196134, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196134 XXXX 1697714196134, Thread 755: XXXX 1697714196134, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
755 1697714196134 XXXX 1697714196134, Thread 755: XXXX 1697714196134, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196134 XXXX 1697714196134, Thread 755: XXXX 1697714196134, Entering Thread 755: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
755 1697714196136 XXXX 1697714196136, Thread 755: XXXX 1697714196136, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196136 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetToolInfo
755 1697714196136 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
755 1697714196136 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
755 1697714196136 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

755 1697714196141 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
755 1697714196141 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
755 1697714196141 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
755 1697714196141 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = erase, Mask = 00000000, Erase = false, Production Mode = true
755 1697714196141 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 0, Type = Pgm, Mask = 00000000
755 1697714196141 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 0, Type = Cfg, Mask = 00000000
755 1697714196141 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc02fef, Buffer Length = 0, Type = BootFlash, Mask = 00000000
755 1697714196141 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
755 1697714196141 XXXX 1697714196141, Thread 755: XXXX 1697714196141, Entering Thread 755: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
755 1697714196148 XXXX 1697714196148, Thread 755: XXXX 1697714196148, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196148 XXXX 1697714196148, Thread 755: XXXX 1697714196148, Entering Thread 755: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
755 1697714196148 XXXX 1697714196148, Thread 755: XXXX 1697714196148, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196148 XXXX 1697714196148, Thread 755: XXXX 1697714196148, Entering Thread 755: Commands::runScriptBasic, script name = EraseChip, timeOut = 30000 ms  
755 1697714196250 XXXX 1697714196250, Thread 755: XXXX 1697714196250, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196250 XXXX 1697714196250, Thread 755: XXXX 1697714196250, Entering Thread 755: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
755 1697714196252 XXXX 1697714196252, Thread 755: XXXX 1697714196252, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196252 XXXX 1697714196252, Thread 755: XXXX 1697714196252, Entering Thread 755: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
755 1697714196259 XXXX 1697714196259, Thread 755: XXXX 1697714196259, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196259 XXXX 1697714196259, Thread 755: XXXX 1697714196259, Entering Thread 755: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
755 1697714196259 XXXX 1697714196259, Thread 755: XXXX 1697714196259, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196259 XXXX 1697714196259, Thread 755: XXXX 1697714196259, Entering Thread 755: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
755 1697714196261 XXXX 1697714196261, Thread 755: XXXX 1697714196261, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196261 XXXX 1697714196261, Thread 755: XXXX 1697714196261, Entering Thread 755: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
755 1697714196262 XXXX 1697714196262, Thread 755: XXXX 1697714196262, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196262 XXXX 1697714196262, Thread 755: XXXX 1697714196262, Entering Thread 755: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
755 1697714196262 XXXX 1697714196262, Thread 755: XXXX 1697714196262, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196262 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
755 1697714196262 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
755 1697714196262 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
755 1697714196262 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

755 1697714196265 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
755 1697714196265 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
755 1697714196265 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
755 1697714196265 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = write, Mask = 00000000, Erase = false, Production Mode = true
755 1697714196265 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 524288, Type = Pgm, Mask = 00000000
755 1697714196265 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 16, Type = Cfg, Mask = 00000000
755 1697714196265 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc01fff, Buffer Length = 8192, Type = BootFlash, Mask = 00000000
755 1697714196265 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
755 1697714196265 XXXX 1697714196265, Thread 755: XXXX 1697714196265, Entering Thread 755: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
755 1697714196266 XXXX 1697714196266, Thread 755: XXXX 1697714196266, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196266 XXXX 1697714196266, Thread 755: XXXX 1697714196266, Entering Thread 755: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
755 1697714196267 XXXX 1697714196267, Thread 755: XXXX 1697714196267, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196267 XXXX 1697714196267, Thread 755: XXXX 1697714196267, Entering Thread 755: Commands::runScriptBasic, script name = SetupSerialMode, timeOut = -1 ms  
755 1697714196269 XXXX 1697714196269, Thread 755: XXXX 1697714196269, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196269 XXXX 1697714196269, Thread 755: XXXX 1697714196269, Entering Thread 755: Commands::runScriptBasic, script name = LoadLoader, timeOut = -1 ms  
755 1697714196295 XXXX 1697714196295, Thread 755: XXXX 1697714196295, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196295 XXXX 1697714196295, Thread 755: XXXX 1697714196295, Entering Thread 755: Commands::runScriptWithDownload, script name = DownloadPE  
755 1697714196365 XXXX 1697714196365, Thread 755: XXXX 1697714196365, Exiting Thread 755: Commands::runScriptWithDownload(DownloadPE)  
755 1697714196365 XXXX 1697714196365, Thread 755: XXXX 1697714196365, Entering Thread 755: Commands::runScriptBasic, script name = TestPEConnect, timeOut = -1 ms  
755 1697714196367 XXXX 1697714196367, Thread 755: XXXX 1697714196367, Exiting Thread 755: Commands::runScriptBasic  
755 1697714196367 XXXX 1697714196367, Thread 755: XXXX 1697714196367, Entering Thread 755: Commands::runScriptWithDownload, script name = WriteProgmemPE  
755 1697714201020 XXXX 1697714201020, Thread 755: com.Send returned false 
760 1697714201021 XXXX 1697714201021, Thread 760: com.Send returned false 
760 1697714201021 XXXX 1697714201021, Thread 760:        ToolCommUsb::DataWriter::run, fatal RI4ControllerException: {null} 
