933 1760620183077 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is null

933 1760620183077 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
933 1760620183077 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
933 1760620183077 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
933 1760620183077 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
933 1760620183078 XXXX 1760620183078, Thread 933: com.Send returned false 
933 1760620183078 XXXX 1760620183078, Thread 933: execCommand: exception after writeSideChanel null 
933 1760620183078 GEN4_CONNECT_DIAGNOSTICS:Removing plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@243f6712
933 1760620183078 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
933 1760620183078 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
933 1760620183128 GEN4_CONNECT_DIAGNOSTICS:Calling RIDbgToolCom.Disconnect
933 1760620183128 GEN4_CONNECT_DIAGNOSTICS:Calling MPLABCommTool.Detach to remove tool from plug and play list
933 1760620183128 GEN4_CONNECT_DIAGNOSTICS:Calling RIDbgToolCom.DisconnectFromMPlabComm
933 1760620183128 GEN4_CONNECT_DIAGNOSTICS:Calling MPLABCommTool.Disconnect
997 1760620258817 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is NOT null
997 1760620258817 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9036, AttachedToolVID = 4d8
997 1760620258817 GEN4_CONNECT_DIAGNOSTICS:transport type = USB
997 1760620258817 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9036, AttachedToolVID = 4d8
997 1760620258822 com.microchip.mplab.mdbcore.RealICETool.RIDbgToolCom
997 1760620258822 GEN4_CONNECT_DIAGNOSTICS:Before MPLABCommTool.Connect()
997 1760620258822 GEN4_CONNECT_DIAGNOSTICS:After MPLABCommTool.Connect()
997 1760620258822 GEN4_CONNECT_DIAGNOSTICS:Adding new plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@7c0a08f2
997 1760620258822 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
997 1760620258822 GEN4_CONNECT_DIAGNOSTICS:com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@7c0a08f2
997 1760620258822 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
997 1760620258822 GEN4_CONNECT_DIAGNOSTICS:Registering for alternate PNP notifications. CommPnPCriteria.cPIDList = [9035], CommPnPCriteria.cSerialNumber = 020026702ryn021743

997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:init
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: Values:
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: pcAddress = 7fffffffffffffff, Vpp = 3.30, useRowEraseIfVoltageIsLow = false, voltageBelowWhichUseRowErase = 0.00, deviceName = PIC32MX695F512H, programmerType = PIC32MX_SSM
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: MemInfo values:
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = ffffffff, exists = true, startAddr = 1d000000, endAddr = 1d07ffff, rowSize = 1000, rowEraseSize = 1000, addrInc = 0004, widthProgram = 0004
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = ffffffff, exists = true, startAddr = 1fc02ff0, endAddr = 1fc02fff, rowSize = 0001, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = true, startAddr = 00000000, endAddr = 00000000, rowSize = 1000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 1000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = ffffffff, exists = true, startAddr = 1f800000, endAddr = 1f88cfff, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 7fffffff, exists = true, startAddr = ffffffff, endAddr = fffffffe, rowSize = 0001, rowEraseSize = 0000, addrInc = 0001, widthProgram = 0001
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: CfgRequiredBitsMask Values:
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ff0, Mask = c307ffff
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ff4, Mask = 00078777
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ff8, Mask = 009ff7a7
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ffc, Mask = 110ff00c
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H BasicInfo: Values:
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H BasicInfo: InputStream = com.microchip.mplab.libs.toolpacksupport.EquatableFileInputStream@cc306916, ToolFlavor = PIC32C
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:init
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H none
997 1760620258841 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4DebugInterface
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4DebugInterfaceImpl@782ffd2f
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ProgramInterface
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ProgramInterfaceImpl@4b6f1b20
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ConnectInterface
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.PK4ToolsController.PK4ConnectInterfaceImpl@670ec727
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ControllerDiagnosticsInterface
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ControllerDiagnosticsInterfaceImpl@7e92f547
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H ProgrammerToGo
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.ProgrammerToGoImpl@79d3b93f
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Status
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H null
997 1760620258842 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SetProgramExec
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H FileRegs
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H a0000900
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Length = 4176
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SetProgramExec
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H true
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK5Tool.PK5Com@2ba30a00
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
997 1760620258852 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
997 1760620258854 XXXX 1760620258854, Thread 997: com.Send returned false 
997 1760620258854 XXXX 1760620258854, Thread 997: execCommand: exception after writeSideChanel null 
