1088 1762126851957 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126851957 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4DebugInterfaceImpl@24f2809f
1088 1762126851957 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1088 1762126851957 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1088 1762126851957 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1088 1762126851957 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ProgramInterface
1088 1762126851957 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126851957 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1088 1762126851957 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126851957 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ProgramInterfaceImpl@153ee5ed
1088 1762126851957 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ConnectInterface
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.PK4ToolsController.PK4ConnectInterfaceImpl@2d5c8bc1
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End
1088 1762126851958 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]
1088 1762126851958 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
1088 1762126851958 GEN4_CONNECT_DIAGNOSTICS:Setting selected tool type to pk4
1088 1762126851958 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
1088 1762126851958 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]

1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ControllerDiagnosticsInterface
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ControllerDiagnosticsInterfaceImpl@395481d3
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H ProgrammerToGo
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.ProgrammerToGoImpl@992081e
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Status
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H null
1088 1762126851958 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SetProgramExec
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H FileRegs
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H a0000900
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Length = 4176
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SetProgramExec
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H true
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@6b61954c
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:uMode = checkingVersions
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:Parsing file  for firmware updates
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ParseSelectedVersionsFromJamFile()
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:Jame file line = boot.hex,010000
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:Jame file line = scripts.xml,000671
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app1 020135, 0040C000
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app2 1.15.20, 00500000
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app3 000000, FFFFFFFF
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app4 000000, FFFFFFFF
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app5 000000, FFFFFFFF
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app6 000000, FFFFFFFF
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app7 000000, FFFFFFFF
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app8 000000, FFFFFFFF
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ri4ParseSelectedVersionsFromJamFile()
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
1088 1762126851970 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4

1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@10527c12
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1088 1762126851970 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126851977 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
1088 1762126851977 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126851977 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
1088 1762126851977 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
1088 1762126851977 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
1088 1762126851994 GEN4_CONNECT_DIAGNOSTICS:appNeedsUpdate returned false
1088 1762126851994 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

1088 1762126851994 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
1088 1762126851994 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1088 1762126851994 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@10527c12
1088 1762126851994 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126851995 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
1088 1762126851995 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126851995 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
1088 1762126851995 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1088 1762126851995 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
1088 1762126851995 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1088 1762126851995 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1088 1762126851995 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126852002 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
1088 1762126852002 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126852002 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
1088 1762126852002 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
1088 1762126852002 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1088 1762126852002 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
1088 1762126852002 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1088 1762126852002 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1088 1762126852002 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126852010 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
1088 1762126852010 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126852010 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
1088 1762126852010 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
1088 1762126852010 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
1088 1762126852010 XXXX 1762126852010, Thread 1088: XXXX 1762126852010, Entering Thread 1088: Commands::runScriptWithUpload with script contents. contents[0] = 0x5e, ...  
1088 1762126852010 XXXX 1762126852010, Thread 1088: XXXX 1762126852010, Entering Thread 1088: ToolCommUsb::readTransfer, sideData is 0xd bytes long, transferDataLength is 0x4 bytes long  
1088 1762126852012 XXXX 1762126852012, Thread 1088: XXXX 1762126852012, Exiting Thread 1088: ToolCommUsb::readTransfer,  cr.status = 0x0  
1088 1762126852012 XXXX 1762126852012, Thread 1088: XXXX 1762126852012, Exiting Thread 1088: Commands::runScriptWithUpload  
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@6b61954c
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:uMode = done
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:Don't upgrade fimware = false
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
1088 1762126852012 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

1088 1762126852012 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetPowerInfo
1088 1762126852012 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1088 1762126852012 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: Values:
1088 1762126852012 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: shotDownSystem = false, isToolPower = true, voltage = 3.250000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
1088 1762126852012 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126852012 XXXX 1762126852012, Thread 1088: XXXX 1762126852012, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
1088 1762126852013 XXXX 1762126852013, Thread 1088: XXXX 1762126852013, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852013 XXXX 1762126852013, Thread 1088: XXXX 1762126852013, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
1088 1762126852014 XXXX 1762126852014, Thread 1088: XXXX 1762126852014, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852014 XXXX 1762126852014, Thread 1088: XXXX 1762126852014, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
1088 1762126852026 XXXX 1762126852026, Thread 1088: XXXX 1762126852026, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852026 XXXX 1762126852026, Thread 1088: XXXX 1762126852026, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
1088 1762126852203 XXXX 1762126852203, Thread 1088: XXXX 1762126852203, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852203 XXXX 1762126852203, Thread 1088: XXXX 1762126852203, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
1088 1762126852208 XXXX 1762126852208, Thread 1088: XXXX 1762126852208, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852208 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetPowerInfo
1088 1762126852208 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126852208 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
1088 1762126852208 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1088 1762126852208 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetLEDBrightness
1088 1762126852208 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1088 1762126852208 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H 5
1088 1762126852208 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126852208 XXXX 1762126852208, Thread 1088: XXXX 1762126852208, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0xcf, ...  
1088 1762126852209 XXXX 1762126852209, Thread 1088: XXXX 1762126852209, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852209 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetLEDBrightness
1088 1762126852209 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126852209 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
1088 1762126852209 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1088 1762126852209 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetToolInfo
1088 1762126852209 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1088 1762126852209 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: Values:
1088 1762126852209 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: speedLevel = 0, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
1088 1762126852209 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126852209 XXXX 1762126852209, Thread 1088: XXXX 1762126852209, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
1088 1762126852209 XXXX 1762126852209, Thread 1088: XXXX 1762126852209, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852210 XXXX 1762126852210, Thread 1088: XXXX 1762126852210, Entering Thread 1088: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
1088 1762126852210 XXXX 1762126852210, Thread 1088: XXXX 1762126852210, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852210 XXXX 1762126852210, Thread 1088: XXXX 1762126852210, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
1088 1762126852211 XXXX 1762126852211, Thread 1088: XXXX 1762126852211, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852211 XXXX 1762126852211, Thread 1088: XXXX 1762126852211, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0xec, ...  
1088 1762126852212 XXXX 1762126852212, Thread 1088: XXXX 1762126852212, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852212 XXXX 1762126852212, Thread 1088: XXXX 1762126852212, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
1088 1762126852213 XXXX 1762126852213, Thread 1088: XXXX 1762126852213, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852213 XXXX 1762126852213, Thread 1088: XXXX 1762126852213, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
1088 1762126852214 XXXX 1762126852214, Thread 1088: XXXX 1762126852214, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852214 XXXX 1762126852214, Thread 1088: XXXX 1762126852214, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
1088 1762126852216 XXXX 1762126852216, Thread 1088: XXXX 1762126852216, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852216 XXXX 1762126852216, Thread 1088: XXXX 1762126852216, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
1088 1762126852216 XXXX 1762126852216, Thread 1088: XXXX 1762126852216, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852216 XXXX 1762126852216, Thread 1088: XXXX 1762126852216, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
1088 1762126852218 XXXX 1762126852218, Thread 1088: XXXX 1762126852218, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852218 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetToolInfo
1088 1762126852218 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126852218 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
1088 1762126852218 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1088 1762126852219 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetTargetIDInfo
1088 1762126852219 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1088 1762126852219 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1088 1762126852219 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126852221 XXXX 1762126852221, Thread 1088: XXXX 1762126852221, Entering Thread 1088: Commands::runScriptBasic, script name = ReadDeviceParameters, timeOut = -1 ms  
1088 1762126852222 XXXX 1762126852222, Thread 1088: XXXX 1762126852222, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852222 XXXX 1762126852222, Thread 1088: XXXX 1762126852222, Entering Thread 1088: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
1088 1762126852228 XXXX 1762126852228, Thread 1088: XXXX 1762126852228, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852229 XXXX 1762126852228, Thread 1088: XXXX 1762126852228, Entering Thread 1088: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
1088 1762126852229 XXXX 1762126852229, Thread 1088: XXXX 1762126852229, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852229 XXXX 1762126852229, Thread 1088: XXXX 1762126852229, Entering Thread 1088: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
1088 1762126852230 XXXX 1762126852230, Thread 1088: XXXX 1762126852230, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852231 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetTargetIDInfo
1088 1762126852231 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126852231 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H TargetIDInfo: Values:
1088 1762126852231 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H TargetIDInfo: DeviceID = 54325053
1088 1762126852231 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1088 1762126852246 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
1088 1762126852246 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
1088 1762126852246 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
1088 1762126852246 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = erase, Mask = 00000000, Erase = false, Production Mode = true
1088 1762126852246 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 0, Type = Pgm, Mask = 00000000
1088 1762126852246 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 0, Type = Cfg, Mask = 00000000
1088 1762126852246 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc02fef, Buffer Length = 0, Type = BootFlash, Mask = 00000000
1088 1762126852246 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
1088 1762126852246 XXXX 1762126852246, Thread 1088: XXXX 1762126852246, Entering Thread 1088: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
1088 1762126852252 XXXX 1762126852252, Thread 1088: XXXX 1762126852252, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852252 XXXX 1762126852252, Thread 1088: XXXX 1762126852252, Entering Thread 1088: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
1088 1762126852252 XXXX 1762126852252, Thread 1088: XXXX 1762126852252, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852252 XXXX 1762126852252, Thread 1088: XXXX 1762126852252, Entering Thread 1088: Commands::runScriptBasic, script name = EraseChip, timeOut = 30000 ms  
1088 1762126852355 XXXX 1762126852355, Thread 1088: XXXX 1762126852355, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852355 XXXX 1762126852355, Thread 1088: XXXX 1762126852355, Entering Thread 1088: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
1088 1762126852357 XXXX 1762126852357, Thread 1088: XXXX 1762126852357, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852357 XXXX 1762126852357, Thread 1088: XXXX 1762126852357, Entering Thread 1088: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
1088 1762126852363 XXXX 1762126852363, Thread 1088: XXXX 1762126852363, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852363 XXXX 1762126852363, Thread 1088: XXXX 1762126852363, Entering Thread 1088: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
1088 1762126852363 XXXX 1762126852363, Thread 1088: XXXX 1762126852363, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852363 XXXX 1762126852363, Thread 1088: XXXX 1762126852363, Entering Thread 1088: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
1088 1762126852365 XXXX 1762126852365, Thread 1088: XXXX 1762126852365, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852365 XXXX 1762126852365, Thread 1088: XXXX 1762126852365, Entering Thread 1088: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
1088 1762126852366 XXXX 1762126852366, Thread 1088: XXXX 1762126852366, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852366 XXXX 1762126852366, Thread 1088: XXXX 1762126852366, Entering Thread 1088: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
1088 1762126852366 XXXX 1762126852366, Thread 1088: XXXX 1762126852366, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852366 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
1088 1762126852366 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
1088 1762126852366 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
1088 1762126852366 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

1088 1762126852372 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
1088 1762126852372 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
1088 1762126852372 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
1088 1762126852372 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = write, Mask = 00000000, Erase = false, Production Mode = true
1088 1762126852372 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 524288, Type = Pgm, Mask = 00000000
1088 1762126852372 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 16, Type = Cfg, Mask = 00000000
1088 1762126852372 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc01fff, Buffer Length = 8192, Type = BootFlash, Mask = 00000000
1088 1762126852372 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
1088 1762126852372 XXXX 1762126852372, Thread 1088: XXXX 1762126852372, Entering Thread 1088: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
1088 1762126852373 XXXX 1762126852373, Thread 1088: XXXX 1762126852373, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852373 XXXX 1762126852373, Thread 1088: XXXX 1762126852373, Entering Thread 1088: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
1088 1762126852373 XXXX 1762126852373, Thread 1088: XXXX 1762126852373, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852373 XXXX 1762126852373, Thread 1088: XXXX 1762126852373, Entering Thread 1088: Commands::runScriptBasic, script name = SetupSerialMode, timeOut = -1 ms  
1088 1762126852375 XXXX 1762126852375, Thread 1088: XXXX 1762126852375, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852375 XXXX 1762126852375, Thread 1088: XXXX 1762126852375, Entering Thread 1088: Commands::runScriptBasic, script name = LoadLoader, timeOut = -1 ms  
1088 1762126852420 XXXX 1762126852420, Thread 1088: XXXX 1762126852420, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852420 XXXX 1762126852420, Thread 1088: XXXX 1762126852420, Entering Thread 1088: Commands::runScriptWithDownload, script name = DownloadPE  
1088 1762126852546 XXXX 1762126852546, Thread 1088: XXXX 1762126852546, Exiting Thread 1088: Commands::runScriptWithDownload(DownloadPE)  
1088 1762126852546 XXXX 1762126852546, Thread 1088: XXXX 1762126852546, Entering Thread 1088: Commands::runScriptBasic, script name = TestPEConnect, timeOut = -1 ms  
1088 1762126852546 XXXX 1762126852546, Thread 1088: XXXX 1762126852546, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126852547 XXXX 1762126852546, Thread 1088: XXXX 1762126852546, Entering Thread 1088: Commands::runScriptWithDownload, script name = WriteProgmemPE  
1088 1762126868277 XXXX 1762126868277, Thread 1088: XXXX 1762126868277, Exiting Thread 1088: Commands::runScriptWithDownload(WriteProgmemPE)  
1088 1762126868277 XXXX 1762126868277, Thread 1088: XXXX 1762126868277, Entering Thread 1088: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
1088 1762126868342 XXXX 1762126868342, Thread 1088: XXXX 1762126868342, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126868343 XXXX 1762126868343, Thread 1088: XXXX 1762126868343, Entering Thread 1088: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
1088 1762126868406 XXXX 1762126868406, Thread 1088: XXXX 1762126868406, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126868407 XXXX 1762126868407, Thread 1088: XXXX 1762126868407, Entering Thread 1088: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
1088 1762126868470 XXXX 1762126868470, Thread 1088: XXXX 1762126868470, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126868471 XXXX 1762126868471, Thread 1088: XXXX 1762126868471, Entering Thread 1088: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
1088 1762126868534 XXXX 1762126868534, Thread 1088: XXXX 1762126868534, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126868535 XXXX 1762126868535, Thread 1088: XXXX 1762126868535, Entering Thread 1088: Commands::runScriptWithDownload, script name = WriteConfigmemPE  
1088 1762126868537 XXXX 1762126868537, Thread 1088: XXXX 1762126868537, Exiting Thread 1088: Commands::runScriptWithDownload(WriteConfigmemPE)  
1088 1762126868537 XXXX 1762126868537, Thread 1088: XXXX 1762126868537, Entering Thread 1088: Commands::runScriptWithUpload, script name = ReadProgmemPE  
1088 1762126868537 XXXX 1762126868537, Thread 1088: XXXX 1762126868537, Entering Thread 1088: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x10 bytes long  
1088 1762126868540 XXXX 1762126868540, Thread 1088: XXXX 1762126868540, Exiting Thread 1088: ToolCommUsb::readTransfer,  cr.status = 0x0  
1088 1762126868540 XXXX 1762126868540, Thread 1088: XXXX 1762126868540, Exiting Thread 1088: Commands::runScriptWithUpload  
1088 1762126868540 XXXX 1762126868540, Thread 1088: XXXX 1762126868540, Entering Thread 1088: Commands::runScriptWithDownload, script name = WriteProgmemPE  
1088 1762126868791 XXXX 1762126868791, Thread 1088: XXXX 1762126868791, Exiting Thread 1088: Commands::runScriptWithDownload(WriteProgmemPE)  
1088 1762126868791 XXXX 1762126868791, Thread 1088: XXXX 1762126868791, Entering Thread 1088: Commands::runScriptWithUpload, script name = ReadProgmemPE  
1088 1762126868791 XXXX 1762126868791, Thread 1088: XXXX 1762126868791, Entering Thread 1088: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x2000 bytes long  
1088 1762126869037 XXXX 1762126869037, Thread 1088: XXXX 1762126869037, Exiting Thread 1088: ToolCommUsb::readTransfer,  cr.status = 0x0  
1088 1762126869037 XXXX 1762126869037, Thread 1088: XXXX 1762126869037, Exiting Thread 1088: Commands::runScriptWithUpload  
1088 1762126869037 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
1088 1762126869037 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
1088 1762126869037 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
1088 1762126869037 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

1088 1762126869037 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:endOfOperations
1088 1762126869037 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
1088 1762126869037 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H null
1088 1762126869037 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
1088 1762126869037 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:endOfOperations
1088 1762126869037 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
1088 1762126869037 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
1088 1762126869037 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

1088 1762126869040 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
1088 1762126869040 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
1088 1762126869040 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
1088 1762126869040 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = releasefromreset, Mask = 00000000, Erase = false, Production Mode = true
1088 1762126869040 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
1088 1762126869040 XXXX 1762126869040, Thread 1088: XXXX 1762126869040, Entering Thread 1088: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
1088 1762126869043 XXXX 1762126869043, Thread 1088: XXXX 1762126869043, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126869043 XXXX 1762126869043, Thread 1088: XXXX 1762126869043, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0x42, ...  
1088 1762126869044 XXXX 1762126869044, Thread 1088: XXXX 1762126869044, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126869044 XXXX 1762126869044, Thread 1088: XXXX 1762126869044, Entering Thread 1088: Commands::runScriptBasic with script contents. contents[0] = 0xef, ...  
1088 1762126869055 XXXX 1762126869055, Thread 1088: XXXX 1762126869055, Exiting Thread 1088: Commands::runScriptBasic  
1088 1762126869055 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
1088 1762126869055 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
1088 1762126869055 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
1088 1762126869055 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End
1088 1762126869055 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is null

1088 1762126869055 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
1088 1762126869055 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1088 1762126869055 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1088 1762126869055 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1088 1762126869062 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
1088 1762126869062 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1088 1762126869062 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
1088 1762126869063 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
1088 1762126869063 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
1088 1762126869063 GEN4_CONNECT_DIAGNOSTICS:Removing plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@20a7494c
1088 1762126869063 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
1088 1762126869063 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
1088 1762126869113 GEN4_CONNECT_DIAGNOSTICS:Calling RIDbgToolCom.Disconnect
1088 1762126869113 GEN4_CONNECT_DIAGNOSTICS:Calling MPLABCommTool.Detach to remove tool from plug and play list
1088 1762126869113 GEN4_CONNECT_DIAGNOSTICS:Calling RIDbgToolCom.DisconnectFromMPlabComm
1088 1762126869113 GEN4_CONNECT_DIAGNOSTICS:Calling MPLABCommTool.Disconnect
1111 1762126951301 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is NOT null
1111 1762126951301 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9012, AttachedToolVID = 4d8
1111 1762126951301 GEN4_CONNECT_DIAGNOSTICS:transport type = USB
1111 1762126951301 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9012, AttachedToolVID = 4d8
1111 1762126951305 com.microchip.mplab.mdbcore.RealICETool.RIDbgToolCom
1111 1762126951305 GEN4_CONNECT_DIAGNOSTICS:Before MPLABCommTool.Connect()
1111 1762126951305 GEN4_CONNECT_DIAGNOSTICS:After MPLABCommTool.Connect()
1111 1762126951305 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool.Connect() returned MPLABCOMM_NO_ERROR
1111 1762126951305 GEN4_CONNECT_DIAGNOSTICS:Attaching to MPLABCommTool plugnplay
1111 1762126951305 GEN4_CONNECT_DIAGNOSTICS:Adding new plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@71651402
1111 1762126951305 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
1111 1762126951305 GEN4_CONNECT_DIAGNOSTICS:com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@71651402
1111 1762126951305 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
1111 1762126951305 GEN4_CONNECT_DIAGNOSTICS:Registering for alternate PNP notifications. CommPnPCriteria.cPIDList = [2177, 2179, 217a, 2141, 9017, 901b, 9036, 9035], CommPnPCriteria.cSerialNumber = bur213375184

1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:init
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: Values:
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: pcAddress = 7fffffffffffffff, Vpp = 3.30, useRowEraseIfVoltageIsLow = false, voltageBelowWhichUseRowErase = 0.00, deviceName = PIC32MX695F512H, programmerType = PIC32MX_SSM
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: MemInfo values:
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = ffffffff, exists = true, startAddr = 1d000000, endAddr = 1d07ffff, rowSize = 1000, rowEraseSize = 1000, addrInc = 0004, widthProgram = 0004
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = ffffffff, exists = true, startAddr = 1fc02ff0, endAddr = 1fc02fff, rowSize = 0001, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = true, startAddr = 00000000, endAddr = 00000000, rowSize = 1000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 1000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = ffffffff, exists = true, startAddr = 1f800000, endAddr = 1f88cfff, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 7fffffff, exists = true, startAddr = ffffffff, endAddr = fffffffe, rowSize = 0001, rowEraseSize = 0000, addrInc = 0001, widthProgram = 0001
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: CfgRequiredBitsMask Values:
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ff0, Mask = c307ffff
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ff4, Mask = 00078777
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ff8, Mask = 009ff7a7
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ffc, Mask = 110ff00c
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H BasicInfo: Values:
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H BasicInfo: InputStream = com.microchip.mplab.libs.toolpacksupport.EquatableFileInputStream@1fa17626, ToolFlavor = PICKit4
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:init
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H none
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4DebugInterface
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4DebugInterfaceImpl@7a6b6c9
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ProgramInterface
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ProgramInterfaceImpl@2cb7dd46
1111 1762126951322 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ConnectInterface
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.PK4ToolsController.PK4ConnectInterfaceImpl@752b09d6
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End
1111 1762126951323 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]
1111 1762126951323 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
1111 1762126951323 GEN4_CONNECT_DIAGNOSTICS:Setting selected tool type to pk4
1111 1762126951323 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
1111 1762126951323 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]

1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ControllerDiagnosticsInterface
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ControllerDiagnosticsInterfaceImpl@49a63494
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H ProgrammerToGo
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.ProgrammerToGoImpl@7b04c397
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Status
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H null
1111 1762126951323 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1111 1762126951336 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SetProgramExec
1111 1762126951336 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
1111 1762126951336 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H FileRegs
1111 1762126951336 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H a0000900
1111 1762126951336 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Length = 4176
1111 1762126951336 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951336 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SetProgramExec
1111 1762126951336 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951336 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H true
1111 1762126951336 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End
1111 1762126951336 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
1111 1762126951336 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@694b7c5c
1111 1762126951336 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
1111 1762126951336 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
1111 1762126951336 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
1111 1762126951336 GEN4_CONNECT_DIAGNOSTICS:uMode = checkingVersions
1111 1762126951336 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
1111 1762126951336 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
1111 1762126951336 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
1111 1762126951336 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
1111 1762126951336 GEN4_CONNECT_DIAGNOSTICS:Parsing file  for firmware updates
1111 1762126951336 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ParseSelectedVersionsFromJamFile()
1111 1762126951336 GEN4_CONNECT_DIAGNOSTICS:Jame file line = boot.hex,010000
1111 1762126951337 GEN4_CONNECT_DIAGNOSTICS:Jame file line = scripts.xml,000671
1111 1762126951337 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app1 020135, 0040C000
1111 1762126951337 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app2 1.15.20, 00500000
1111 1762126951337 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app3 000000, FFFFFFFF
1111 1762126951337 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app4 000000, FFFFFFFF
1111 1762126951337 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app5 000000, FFFFFFFF
1111 1762126951337 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app6 000000, FFFFFFFF
1111 1762126951337 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app7 000000, FFFFFFFF
1111 1762126951337 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app8 000000, FFFFFFFF
1111 1762126951337 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ri4ParseSelectedVersionsFromJamFile()
1111 1762126951337 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
1111 1762126951337 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4

1111 1762126951337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
1111 1762126951337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@20915ff7
1111 1762126951337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
1111 1762126951337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
1111 1762126951337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1111 1762126951337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
1111 1762126951337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1111 1762126951337 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951344 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
1111 1762126951344 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951344 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
1111 1762126951344 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
1111 1762126951344 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
1111 1762126951361 GEN4_CONNECT_DIAGNOSTICS:appNeedsUpdate returned false
1111 1762126951361 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

1111 1762126951361 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
1111 1762126951361 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951361 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@20915ff7
1111 1762126951361 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951362 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
1111 1762126951362 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951362 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
1111 1762126951362 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1111 1762126951362 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
1111 1762126951362 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951362 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1111 1762126951362 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951369 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
1111 1762126951369 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951369 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
1111 1762126951369 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
1111 1762126951369 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1111 1762126951369 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
1111 1762126951369 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951369 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1111 1762126951369 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951375 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
1111 1762126951375 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951375 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
1111 1762126951375 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
1111 1762126951375 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
1111 1762126951375 XXXX 1762126951375, Thread 1111: XXXX 1762126951375, Entering Thread 1111: Commands::runScriptWithUpload with script contents. contents[0] = 0x5e, ...  
1111 1762126951375 XXXX 1762126951375, Thread 1111: XXXX 1762126951375, Entering Thread 1111: ToolCommUsb::readTransfer, sideData is 0xd bytes long, transferDataLength is 0x4 bytes long  
1111 1762126951377 XXXX 1762126951377, Thread 1111: XXXX 1762126951377, Exiting Thread 1111: ToolCommUsb::readTransfer,  cr.status = 0x0  
1111 1762126951377 XXXX 1762126951377, Thread 1111: XXXX 1762126951377, Exiting Thread 1111: Commands::runScriptWithUpload  
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@694b7c5c
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:uMode = done
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:Don't upgrade fimware = false
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
1111 1762126951377 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

1111 1762126951377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetPowerInfo
1111 1762126951377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: Values:
1111 1762126951377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: shotDownSystem = false, isToolPower = true, voltage = 3.250000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
1111 1762126951377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951377 XXXX 1762126951377, Thread 1111: XXXX 1762126951377, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
1111 1762126951378 XXXX 1762126951378, Thread 1111: XXXX 1762126951378, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951378 XXXX 1762126951378, Thread 1111: XXXX 1762126951378, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
1111 1762126951379 XXXX 1762126951379, Thread 1111: XXXX 1762126951379, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951379 XXXX 1762126951379, Thread 1111: XXXX 1762126951379, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
1111 1762126951392 XXXX 1762126951392, Thread 1111: XXXX 1762126951392, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951392 XXXX 1762126951392, Thread 1111: XXXX 1762126951392, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
1111 1762126951569 XXXX 1762126951569, Thread 1111: XXXX 1762126951569, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951569 XXXX 1762126951569, Thread 1111: XXXX 1762126951569, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
1111 1762126951574 XXXX 1762126951574, Thread 1111: XXXX 1762126951574, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951574 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetPowerInfo
1111 1762126951574 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951574 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
1111 1762126951574 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1111 1762126951574 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetLEDBrightness
1111 1762126951574 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951574 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H 5
1111 1762126951574 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951574 XXXX 1762126951574, Thread 1111: XXXX 1762126951574, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0xcf, ...  
1111 1762126951575 XXXX 1762126951575, Thread 1111: XXXX 1762126951575, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951575 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetLEDBrightness
1111 1762126951575 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951575 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
1111 1762126951575 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1111 1762126951575 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetToolInfo
1111 1762126951575 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951575 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: Values:
1111 1762126951575 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: speedLevel = 0, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
1111 1762126951575 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951575 XXXX 1762126951575, Thread 1111: XXXX 1762126951575, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
1111 1762126951575 XXXX 1762126951575, Thread 1111: XXXX 1762126951575, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951575 XXXX 1762126951575, Thread 1111: XXXX 1762126951575, Entering Thread 1111: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
1111 1762126951576 XXXX 1762126951576, Thread 1111: XXXX 1762126951576, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951576 XXXX 1762126951576, Thread 1111: XXXX 1762126951576, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
1111 1762126951577 XXXX 1762126951577, Thread 1111: XXXX 1762126951577, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951577 XXXX 1762126951577, Thread 1111: XXXX 1762126951577, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0xec, ...  
1111 1762126951578 XXXX 1762126951578, Thread 1111: XXXX 1762126951578, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951578 XXXX 1762126951578, Thread 1111: XXXX 1762126951578, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
1111 1762126951579 XXXX 1762126951579, Thread 1111: XXXX 1762126951579, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951579 XXXX 1762126951579, Thread 1111: XXXX 1762126951579, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
1111 1762126951580 XXXX 1762126951580, Thread 1111: XXXX 1762126951580, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951580 XXXX 1762126951580, Thread 1111: XXXX 1762126951580, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
1111 1762126951581 XXXX 1762126951581, Thread 1111: XXXX 1762126951581, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951581 XXXX 1762126951581, Thread 1111: XXXX 1762126951581, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
1111 1762126951582 XXXX 1762126951582, Thread 1111: XXXX 1762126951582, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951582 XXXX 1762126951582, Thread 1111: XXXX 1762126951582, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
1111 1762126951583 XXXX 1762126951583, Thread 1111: XXXX 1762126951583, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951583 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetToolInfo
1111 1762126951583 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951583 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
1111 1762126951583 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1111 1762126951585 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetTargetIDInfo
1111 1762126951585 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1111 1762126951585 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1111 1762126951585 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951587 XXXX 1762126951587, Thread 1111: XXXX 1762126951587, Entering Thread 1111: Commands::runScriptBasic, script name = ReadDeviceParameters, timeOut = -1 ms  
1111 1762126951588 XXXX 1762126951588, Thread 1111: XXXX 1762126951588, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951588 XXXX 1762126951588, Thread 1111: XXXX 1762126951588, Entering Thread 1111: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
1111 1762126951595 XXXX 1762126951595, Thread 1111: XXXX 1762126951595, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951595 XXXX 1762126951595, Thread 1111: XXXX 1762126951595, Entering Thread 1111: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
1111 1762126951596 XXXX 1762126951596, Thread 1111: XXXX 1762126951596, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951596 XXXX 1762126951596, Thread 1111: XXXX 1762126951596, Entering Thread 1111: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
1111 1762126951597 XXXX 1762126951597, Thread 1111: XXXX 1762126951597, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951597 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetTargetIDInfo
1111 1762126951597 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951597 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H TargetIDInfo: Values:
1111 1762126951597 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H TargetIDInfo: DeviceID = 54325053
1111 1762126951597 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1111 1762126951613 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
1111 1762126951613 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
1111 1762126951613 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
1111 1762126951613 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = erase, Mask = 00000000, Erase = false, Production Mode = true
1111 1762126951613 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 0, Type = Pgm, Mask = 00000000
1111 1762126951613 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 0, Type = Cfg, Mask = 00000000
1111 1762126951613 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc02fef, Buffer Length = 0, Type = BootFlash, Mask = 00000000
1111 1762126951613 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951613 XXXX 1762126951613, Thread 1111: XXXX 1762126951613, Entering Thread 1111: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
1111 1762126951619 XXXX 1762126951619, Thread 1111: XXXX 1762126951619, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951619 XXXX 1762126951619, Thread 1111: XXXX 1762126951619, Entering Thread 1111: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
1111 1762126951619 XXXX 1762126951619, Thread 1111: XXXX 1762126951619, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951619 XXXX 1762126951619, Thread 1111: XXXX 1762126951619, Entering Thread 1111: Commands::runScriptBasic, script name = EraseChip, timeOut = 30000 ms  
1111 1762126951721 XXXX 1762126951721, Thread 1111: XXXX 1762126951721, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951721 XXXX 1762126951721, Thread 1111: XXXX 1762126951721, Entering Thread 1111: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
1111 1762126951723 XXXX 1762126951723, Thread 1111: XXXX 1762126951723, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951723 XXXX 1762126951723, Thread 1111: XXXX 1762126951723, Entering Thread 1111: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
1111 1762126951729 XXXX 1762126951729, Thread 1111: XXXX 1762126951729, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951729 XXXX 1762126951729, Thread 1111: XXXX 1762126951729, Entering Thread 1111: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
1111 1762126951730 XXXX 1762126951730, Thread 1111: XXXX 1762126951730, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951730 XXXX 1762126951730, Thread 1111: XXXX 1762126951730, Entering Thread 1111: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
1111 1762126951731 XXXX 1762126951731, Thread 1111: XXXX 1762126951731, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951731 XXXX 1762126951731, Thread 1111: XXXX 1762126951731, Entering Thread 1111: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
1111 1762126951733 XXXX 1762126951733, Thread 1111: XXXX 1762126951733, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951733 XXXX 1762126951733, Thread 1111: XXXX 1762126951733, Entering Thread 1111: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
1111 1762126951734 XXXX 1762126951734, Thread 1111: XXXX 1762126951734, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951734 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
1111 1762126951734 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
1111 1762126951734 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
1111 1762126951734 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

1111 1762126951739 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
1111 1762126951739 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
1111 1762126951739 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
1111 1762126951739 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = write, Mask = 00000000, Erase = false, Production Mode = true
1111 1762126951739 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1d000000, End = 1d07ffff, Buffer Length = 524288, Type = Pgm, Mask = 00000000
1111 1762126951739 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc02ff0, End = 1fc02fff, Buffer Length = 16, Type = Cfg, Mask = 00000000
1111 1762126951739 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H TransferInfo: Start = 1fc00000, End = 1fc01fff, Buffer Length = 8192, Type = BootFlash, Mask = 00000000
1111 1762126951739 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
1111 1762126951739 XXXX 1762126951739, Thread 1111: XXXX 1762126951739, Entering Thread 1111: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
1111 1762126951740 XXXX 1762126951740, Thread 1111: XXXX 1762126951740, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951740 XXXX 1762126951740, Thread 1111: XXXX 1762126951740, Entering Thread 1111: Commands::runScriptBasic, script name = CheckCodeProtect, timeOut = -1 ms  
1111 1762126951740 XXXX 1762126951740, Thread 1111: XXXX 1762126951740, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951740 XXXX 1762126951740, Thread 1111: XXXX 1762126951740, Entering Thread 1111: Commands::runScriptBasic, script name = SetupSerialMode, timeOut = -1 ms  
1111 1762126951742 XXXX 1762126951742, Thread 1111: XXXX 1762126951742, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951742 XXXX 1762126951742, Thread 1111: XXXX 1762126951742, Entering Thread 1111: Commands::runScriptBasic, script name = LoadLoader, timeOut = -1 ms  
1111 1762126951787 XXXX 1762126951787, Thread 1111: XXXX 1762126951787, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951787 XXXX 1762126951787, Thread 1111: XXXX 1762126951787, Entering Thread 1111: Commands::runScriptWithDownload, script name = DownloadPE  
1111 1762126951913 XXXX 1762126951913, Thread 1111: XXXX 1762126951913, Exiting Thread 1111: Commands::runScriptWithDownload(DownloadPE)  
1111 1762126951913 XXXX 1762126951913, Thread 1111: XXXX 1762126951913, Entering Thread 1111: Commands::runScriptBasic, script name = TestPEConnect, timeOut = -1 ms  
1111 1762126951913 XXXX 1762126951913, Thread 1111: XXXX 1762126951913, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126951914 XXXX 1762126951914, Thread 1111: XXXX 1762126951914, Entering Thread 1111: Commands::runScriptWithDownload, script name = WriteProgmemPE  
1111 1762126967657 XXXX 1762126967657, Thread 1111: XXXX 1762126967657, Exiting Thread 1111: Commands::runScriptWithDownload(WriteProgmemPE)  
1111 1762126967657 XXXX 1762126967657, Thread 1111: XXXX 1762126967657, Entering Thread 1111: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
1111 1762126967720 XXXX 1762126967720, Thread 1111: XXXX 1762126967720, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126967721 XXXX 1762126967721, Thread 1111: XXXX 1762126967721, Entering Thread 1111: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
1111 1762126967785 XXXX 1762126967785, Thread 1111: XXXX 1762126967785, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126967785 XXXX 1762126967785, Thread 1111: XXXX 1762126967785, Entering Thread 1111: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
1111 1762126967849 XXXX 1762126967849, Thread 1111: XXXX 1762126967849, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126967849 XXXX 1762126967849, Thread 1111: XXXX 1762126967849, Entering Thread 1111: Commands::runScriptBasic, script name = CalcCRC_PE, timeOut = -1 ms  
1111 1762126967913 XXXX 1762126967913, Thread 1111: XXXX 1762126967913, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126967913 XXXX 1762126967913, Thread 1111: XXXX 1762126967913, Entering Thread 1111: Commands::runScriptWithDownload, script name = WriteConfigmemPE  
1111 1762126967916 XXXX 1762126967916, Thread 1111: XXXX 1762126967916, Exiting Thread 1111: Commands::runScriptWithDownload(WriteConfigmemPE)  
1111 1762126967916 XXXX 1762126967916, Thread 1111: XXXX 1762126967916, Entering Thread 1111: Commands::runScriptWithUpload, script name = ReadProgmemPE  
1111 1762126967916 XXXX 1762126967916, Thread 1111: XXXX 1762126967916, Entering Thread 1111: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x10 bytes long  
1111 1762126967919 XXXX 1762126967919, Thread 1111: XXXX 1762126967919, Exiting Thread 1111: ToolCommUsb::readTransfer,  cr.status = 0x0  
1111 1762126967919 XXXX 1762126967919, Thread 1111: XXXX 1762126967919, Exiting Thread 1111: Commands::runScriptWithUpload  
1111 1762126967919 XXXX 1762126967919, Thread 1111: XXXX 1762126967919, Entering Thread 1111: Commands::runScriptWithDownload, script name = WriteProgmemPE  
1111 1762126968169 XXXX 1762126968169, Thread 1111: XXXX 1762126968169, Exiting Thread 1111: Commands::runScriptWithDownload(WriteProgmemPE)  
1111 1762126968169 XXXX 1762126968169, Thread 1111: XXXX 1762126968169, Entering Thread 1111: Commands::runScriptWithUpload, script name = ReadProgmemPE  
1111 1762126968170 XXXX 1762126968170, Thread 1111: XXXX 1762126968170, Entering Thread 1111: ToolCommUsb::readTransfer, sideData is 0x38 bytes long, transferDataLength is 0x2000 bytes long  
1111 1762126968416 XXXX 1762126968416, Thread 1111: XXXX 1762126968416, Exiting Thread 1111: ToolCommUsb::readTransfer,  cr.status = 0x0  
1111 1762126968416 XXXX 1762126968416, Thread 1111: XXXX 1762126968416, Exiting Thread 1111: Commands::runScriptWithUpload  
1111 1762126968416 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
1111 1762126968416 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
1111 1762126968416 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
1111 1762126968416 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

1111 1762126968416 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:endOfOperations
1111 1762126968416 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
1111 1762126968416 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H null
1111 1762126968416 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
1111 1762126968416 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:endOfOperations
1111 1762126968416 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
1111 1762126968416 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
1111 1762126968416 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End

1111 1762126968420 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SendOperation
1111 1762126968420 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
1111 1762126968420 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Values:
1111 1762126968420 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H OperationInfo: Type = releasefromreset, Mask = 00000000, Erase = false, Production Mode = true
1111 1762126968420 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
1111 1762126968420 XXXX 1762126968420, Thread 1111: XXXX 1762126968420, Entering Thread 1111: Commands::runScriptBasic, script name = ExitTMOD, timeOut = -1 ms  
1111 1762126968422 XXXX 1762126968422, Thread 1111: XXXX 1762126968422, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126968422 XXXX 1762126968422, Thread 1111: XXXX 1762126968422, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0x42, ...  
1111 1762126968423 XXXX 1762126968423, Thread 1111: XXXX 1762126968423, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126968423 XXXX 1762126968423, Thread 1111: XXXX 1762126968423, Entering Thread 1111: Commands::runScriptBasic with script contents. contents[0] = 0xef, ...  
1111 1762126968433 XXXX 1762126968433, Thread 1111: XXXX 1762126968433, Exiting Thread 1111: Commands::runScriptBasic  
1111 1762126968433 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SendOperation
1111 1762126968433 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
1111 1762126968433 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H None
1111 1762126968433 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End
1111 1762126968434 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is null

1111 1762126968434 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
1111 1762126968434 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1111 1762126968434 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1111 1762126968434 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1111 1762126968441 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
1111 1762126968441 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1111 1762126968441 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
1111 1762126968441 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
1111 1762126968441 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
1111 1762126968441 GEN4_CONNECT_DIAGNOSTICS:Removing plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@71651402
1111 1762126968441 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
1111 1762126968441 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
1111 1762126968491 GEN4_CONNECT_DIAGNOSTICS:Calling RIDbgToolCom.Disconnect
1111 1762126968491 GEN4_CONNECT_DIAGNOSTICS:Calling MPLABCommTool.Detach to remove tool from plug and play list
1111 1762126968491 GEN4_CONNECT_DIAGNOSTICS:Calling RIDbgToolCom.DisconnectFromMPlabComm
1111 1762126968491 GEN4_CONNECT_DIAGNOSTICS:Calling MPLABCommTool.Disconnect
1158 1762127131100 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is NOT null
1158 1762127131100 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9012, AttachedToolVID = 4d8
1158 1762127131100 GEN4_CONNECT_DIAGNOSTICS:transport type = USB
1158 1762127131100 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9012, AttachedToolVID = 4d8
1158 1762127131106 com.microchip.mplab.mdbcore.RealICETool.RIDbgToolCom
1158 1762127131106 GEN4_CONNECT_DIAGNOSTICS:Before MPLABCommTool.Connect()
1158 1762127131106 GEN4_CONNECT_DIAGNOSTICS:After MPLABCommTool.Connect()
1158 1762127131106 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool.Connect() returned MPLABCOMM_NO_ERROR
1158 1762127131106 GEN4_CONNECT_DIAGNOSTICS:Attaching to MPLABCommTool plugnplay
1158 1762127131106 GEN4_CONNECT_DIAGNOSTICS:Adding new plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@44471729
1158 1762127131106 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
1158 1762127131106 GEN4_CONNECT_DIAGNOSTICS:com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@44471729
1158 1762127131106 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
1158 1762127131106 GEN4_CONNECT_DIAGNOSTICS:Registering for alternate PNP notifications. CommPnPCriteria.cPIDList = [2177, 2179, 217a, 2141, 9017, 901b, 9036, 9035], CommPnPCriteria.cSerialNumber = bur213375184

1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:init
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: Values:
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: pcAddress = 7fffffffffffffff, Vpp = 3.30, useRowEraseIfVoltageIsLow = false, voltageBelowWhichUseRowErase = 0.00, deviceName = PIC32MX695F512H, programmerType = PIC32MX_SSM
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: MemInfo values:
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = ffffffff, exists = true, startAddr = 1d000000, endAddr = 1d07ffff, rowSize = 1000, rowEraseSize = 1000, addrInc = 0004, widthProgram = 0004
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = ffffffff, exists = true, startAddr = 1fc02ff0, endAddr = 1fc02fff, rowSize = 0001, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = true, startAddr = 00000000, endAddr = 00000000, rowSize = 1000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 1000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = ffffffff, exists = true, startAddr = 1f800000, endAddr = 1f88cfff, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 7fffffff, exists = true, startAddr = ffffffff, endAddr = fffffffe, rowSize = 0001, rowEraseSize = 0000, addrInc = 0001, widthProgram = 0001
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H DeviceInfo: CfgRequiredBitsMask Values:
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ff0, Mask = c307ffff
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ff4, Mask = 00078777
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ff8, Mask = 009ff7a7
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Address = 1fc02ffc, Mask = 110ff00c
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H BasicInfo: Values:
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H BasicInfo: InputStream = com.microchip.mplab.libs.toolpacksupport.EquatableFileInputStream@1fa17626, ToolFlavor = PICKit4
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:init
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H none
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4DebugInterface
1158 1762127131124 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4DebugInterfaceImpl@645f5905
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ProgramInterface
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ProgramInterfaceImpl@3c8b9928
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ConnectInterface
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.PK4ToolsController.PK4ConnectInterfaceImpl@40092fcf
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End
1158 1762127131125 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]
1158 1762127131125 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
1158 1762127131125 GEN4_CONNECT_DIAGNOSTICS:Setting selected tool type to pk4
1158 1762127131125 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2177, 2179, 217a, 2141]
1158 1762127131125 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9012, 9017, 901b, 9036, 9035]

1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H RI4ControllerDiagnosticsInterface
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ControllerDiagnosticsInterfaceImpl@b3b9d04
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H ProgrammerToGo
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H com.microchip.mplab.libs.RI4ToolsController.implementations.ProgrammerToGoImpl@15326a17
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Pre:GetInterfaceProvider
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Status
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Post:GetInterfaceProvider
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H null
1158 1762127131125 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_PIC32MX695F512H Return End

1158 1762127131139 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Pre:SetProgramExec
1158 1762127131139 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload
1158 1762127131139 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H FileRegs
1158 1762127131139 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H a0000900
1158 1762127131139 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Length = 4176
1158 1762127131139 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131139 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Post:SetProgramExec
1158 1762127131139 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131139 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H true
1158 1762127131139 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_PIC32MX695F512H Return End
1158 1762127131139 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
1158 1762127131139 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@7590f340
1158 1762127131139 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
1158 1762127131139 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
1158 1762127131139 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
1158 1762127131139 GEN4_CONNECT_DIAGNOSTICS:uMode = checkingVersions
1158 1762127131139 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
1158 1762127131139 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
1158 1762127131139 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
1158 1762127131139 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:Parsing file  for firmware updates
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ParseSelectedVersionsFromJamFile()
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:Jame file line = boot.hex,010000
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:Jame file line = scripts.xml,000671
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app1 020135, 0040C000
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app2 1.15.20, 00500000
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app3 000000, FFFFFFFF
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app4 000000, FFFFFFFF
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app5 000000, FFFFFFFF
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app6 000000, FFFFFFFF
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app7 000000, FFFFFFFF
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:Jame file line = app8 000000, FFFFFFFF
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ri4ParseSelectedVersionsFromJamFile()
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
1158 1762127131140 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4

1158 1762127131140 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
1158 1762127131140 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131140 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@15864bfb
1158 1762127131140 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131140 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
1158 1762127131140 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131140 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
1158 1762127131140 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1158 1762127131140 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
1158 1762127131140 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131140 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1158 1762127131140 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131147 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
1158 1762127131147 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131147 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
1158 1762127131147 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
1158 1762127131147 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
1158 1762127131163 GEN4_CONNECT_DIAGNOSTICS:appNeedsUpdate returned false
1158 1762127131163 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

1158 1762127131163 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:EstablishCommunincations
1158 1762127131163 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131163 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H com.microchip.mplab.mdbcore.PK4Tool.PK4Com@15864bfb
1158 1762127131163 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131163 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:EstablishCommunincations
1158 1762127131163 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131163 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H true
1158 1762127131163 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1158 1762127131163 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
1158 1762127131163 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131163 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1158 1762127131163 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
1158 1762127131171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
1158 1762127131171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
1158 1762127131171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1158 1762127131171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetFirmwareInfo
1158 1762127131171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1158 1762127131171 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131178 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:GetFirmwareInfo
1158 1762127131178 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131178 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: Values:
1158 1762127131178 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H FirmwareInfo: boot = false, bootVer = 01.00.00, apVer = 02.01.35, fpgaVer = ff.ff.ff, scriptVer = 00.06.71, macAddress = 0495683498072504856485057485049, devID = a1020e01, devID1 = 2, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR213375184, appCommitID = null, scriptCommitID = 74cdf38a4d, PCB_ID = 4
1158 1762127131178 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End
1158 1762127131178 XXXX 1762127131178, Thread 1158: XXXX 1762127131178, Entering Thread 1158: Commands::runScriptWithUpload with script contents. contents[0] = 0x5e, ...  
1158 1762127131178 XXXX 1762127131178, Thread 1158: XXXX 1762127131178, Entering Thread 1158: ToolCommUsb::readTransfer, sideData is 0xd bytes long, transferDataLength is 0x4 bytes long  
1158 1762127131179 XXXX 1762127131179, Thread 1158: XXXX 1762127131179, Exiting Thread 1158: ToolCommUsb::readTransfer,  cr.status = 0x0  
1158 1762127131179 XXXX 1762127131179, Thread 1158: XXXX 1762127131179, Exiting Thread 1158: Commands::runScriptWithUpload  
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@7590f340
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:uMode = done
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:Don't upgrade fimware = false
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
1158 1762127131179 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

1158 1762127131179 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetPowerInfo
1158 1762127131179 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131179 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: Values:
1158 1762127131179 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H PowerInfo: shotDownSystem = false, isToolPower = true, voltage = 3.250000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
1158 1762127131179 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131179 XXXX 1762127131179, Thread 1158: XXXX 1762127131179, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
1158 1762127131182 XXXX 1762127131182, Thread 1158: XXXX 1762127131182, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131182 XXXX 1762127131182, Thread 1158: XXXX 1762127131182, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
1158 1762127131183 XXXX 1762127131183, Thread 1158: XXXX 1762127131183, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131183 XXXX 1762127131183, Thread 1158: XXXX 1762127131183, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
1158 1762127131196 XXXX 1762127131196, Thread 1158: XXXX 1762127131196, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131196 XXXX 1762127131196, Thread 1158: XXXX 1762127131196, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
1158 1762127131373 XXXX 1762127131373, Thread 1158: XXXX 1762127131373, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131373 XXXX 1762127131373, Thread 1158: XXXX 1762127131373, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
1158 1762127131377 XXXX 1762127131377, Thread 1158: XXXX 1762127131377, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetPowerInfo
1158 1762127131377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
1158 1762127131377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1158 1762127131377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetLEDBrightness
1158 1762127131377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H 5
1158 1762127131377 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131377 XXXX 1762127131377, Thread 1158: XXXX 1762127131377, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0xcf, ...  
1158 1762127131378 XXXX 1762127131378, Thread 1158: XXXX 1762127131378, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131378 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetLEDBrightness
1158 1762127131378 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131378 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
1158 1762127131378 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1158 1762127131378 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:SetToolInfo
1158 1762127131378 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131378 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: Values:
1158 1762127131379 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H ToolInfo: speedLevel = 0, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
1158 1762127131379 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131379 XXXX 1762127131379, Thread 1158: XXXX 1762127131379, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
1158 1762127131379 XXXX 1762127131379, Thread 1158: XXXX 1762127131379, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131379 XXXX 1762127131379, Thread 1158: XXXX 1762127131379, Entering Thread 1158: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
1158 1762127131380 XXXX 1762127131380, Thread 1158: XXXX 1762127131380, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131380 XXXX 1762127131380, Thread 1158: XXXX 1762127131380, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
1158 1762127131381 XXXX 1762127131381, Thread 1158: XXXX 1762127131381, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131381 XXXX 1762127131381, Thread 1158: XXXX 1762127131381, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0xec, ...  
1158 1762127131382 XXXX 1762127131382, Thread 1158: XXXX 1762127131382, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131382 XXXX 1762127131382, Thread 1158: XXXX 1762127131382, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
1158 1762127131383 XXXX 1762127131383, Thread 1158: XXXX 1762127131383, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131383 XXXX 1762127131383, Thread 1158: XXXX 1762127131383, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
1158 1762127131384 XXXX 1762127131384, Thread 1158: XXXX 1762127131384, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131384 XXXX 1762127131384, Thread 1158: XXXX 1762127131384, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
1158 1762127131385 XXXX 1762127131385, Thread 1158: XXXX 1762127131385, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131385 XXXX 1762127131385, Thread 1158: XXXX 1762127131385, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
1158 1762127131386 XXXX 1762127131386, Thread 1158: XXXX 1762127131386, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131386 XXXX 1762127131386, Thread 1158: XXXX 1762127131386, Entering Thread 1158: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
1158 1762127131387 XXXX 1762127131387, Thread 1158: XXXX 1762127131387, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131387 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Post:SetToolInfo
1158 1762127131387 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return Value
1158 1762127131387 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H none
1158 1762127131387 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Return End

1158 1762127131390 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Pre:GetTargetIDInfo
1158 1762127131390 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload
1158 1762127131390 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H null
1158 1762127131390 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_PIC32MX695F512H Payload End
1158 1762127131392 XXXX 1762127131392, Thread 1158: XXXX 1762127131392, Entering Thread 1158: Commands::runScriptBasic, script name = ReadDeviceParameters, timeOut = -1 ms  
1158 1762127131393 XXXX 1762127131393, Thread 1158: XXXX 1762127131393, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131393 XXXX 1762127131393, Thread 1158: XXXX 1762127131393, Entering Thread 1158: Commands::runScriptBasic, script name = EnterTMOD_LV, timeOut = -1 ms  
1158 1762127131399 XXXX 1762127131399, Thread 1158: XXXX 1762127131399, Exiting Thread 1158: Commands::runScriptBasic  
1158 1762127131399 XXXX 1762127131399, Thread 1158: XXXX 1762127131399, Entering Thread 1158: Commands::runScriptBasic, script name = InitJTAG, timeOut = -1 ms  
1158 1762127133447 XXXX 1762127133447, Thread 1158: Type = runScript, Script name = InitJTAG, Status = 0x104
 
